REAR 1/4 TRIM FINISH PANEL CORRECTION FOR LOOSE PANEL. Chevrolet Celebrity 1984

For 1990-2009 cars

# REAR 1/4 TRIM FINISH PANEL CORRECTION FOR LOOSE PANEL

#### VEHICLES AFFECTED: All 1984 'A' 19 and 27 Styles

If a loose rear quarter trim finishing panel to fastener is encountered, the condition may be repaired by installing the fastener to the trim panel using an adhesive backed body side moulding foam tape (3M-06380 or equivalent) followed by the installation of cloth-backed waterproof body tape as shown in Figure 1. The cloth-backed body tape is used to provide adequate retention of the fastener to the trim panel and prevent peel load on the tape.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.