NON-REPAIRABLE POLICE- SPEEDOMETERS, REPLACEMENTS. Chevrolet Celebrity 1985

For 1990-2009 cars

# NON-REPAIRABLE POLICE- SPEEDOMETERS, REPLACEMENTS

LATE IN THE 1983 MODEL YEAR, SPECIAL POLICE SPEEDOMETERS WERE RELEASED TO RETAIN CALIBRATION OVER A WIDE RANGE OF TEMPERATURES. THESE SPEEDOMETERS, AND THOSE USED IN SUBSEQUENT MODEL YEARS, WILL NOT BE REPAIRABLE. THE SPECIAL POLICE SPEEDOMETERS RELEASED TO DATE ARE LISTED BELOW: PART NO. APPLICATION 25076605 1983-4 CHEVY B - U.S. - 3 SPD 25077842 1983-4 CHEVY B - U.S. - 4 SPD 25076129 1984-5 CHEVY A - U.S. 25076130 1984-5 CHEVY A - CANADIAN 25078352 1985 CHEVY B - U.S. 25078353 1985 CHEVY B - CANADIAN THESE SPEEDOMETERS MUST BE REPLACED AS ASSEMBLIES, RATHER THAN REPAIRED BY COMPONENTS. WHEN REPLACED, THE ODOMETERS SHOULD NOT BE RESET TO ACTUAL VEHICLE MILEAGE. (TO DO SO WOULD DESTROY CALIBRATION.) STICKERS SHOULD BE AFFIXED TO DRIVERS' DOORS INDICATING MILEAGE AT THE TIME OF SPEEDOMETER REPLACEMENT.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.