Technical Service Bulletins Chevrolet Celebrity 1985

For 1990-2009 cars

# Technical Service Bulletins

- 2008-06-04: No Movement When Transmission is Shifted to Drive or Third - Normal Operation When Shifted to Second, First or Reverse (Replace Forward Sprag Assembly) (08-07-30-027)
- 2008-04-04: 4L60 Automatic Transmission - New Sprag Assembly, Forward Clutch to Overrun Clutch Hub (08-07-30-017)
- 2006-01-27: Service VME - Use Correct Engine Oil Drain Plug - keywords drain engine leak oil pan plug replace (PIP3696)
- 2006-01-18: Info - New Product Feedback Form and Process for Automatic Transmission Core Returns (01-07-30-029A)
- 2004-03-18: No TCC Apply , MIL On , TCC Surge , Possible P0740 , P1870 , or 39 after Installation of Reman ( SRTA ) 4T60 / 4T60E - kw case cover converter slip transmission (PI01880A)
- 1997-12-11: WARRANTY ADMIN - ACDELCO REMANUFACTURED ENGINES (72-05-07)
- 1997-01-01: GUIDELINES FOR RETROFITTING R-12 VEH. TO R-134A (43-12-07E)
- 1996-12-01: SERVICE ADMINISTRATION - WARRANTY CLAIMS PROCESSING (31-05-03C)
- 1995-10-10: WARRANTY INFORMATION ALL MODELS - ALL YEARS (58-05-03)
- 1995-10-09: INFO. ON DAYTIME RUNNING LAMPS (DRL) (53-82-09)
- 1995-10-01: CAMPAIGN: SERVICE PART FUEL TANK SENDER RING WELDS (91-C-51A)
- 1995-09-01: REPLACEMENT OF ISOLATION DIODES (93-163-8A)
- 1995-06-12: INFO. ON REFORMULATED GASOLINE (RFG) (57-01-02)
- 1995-06-01: CAMPAIGN: SERVICE PART FUEL TANK SENDER RING WELDS (91-C-51)
- 1995-04-27: INFORMATION ON GM CAMPAIGN IDENTIFICATION LABEL (51-01-03)
- 1995-04-01: INFORMATION ON SIERRA-BRAND ENGINE COOLANT (43-62-01B)
- 1995-03-01: SMU - SECTION 3D - LOWER MOUNTING BOLT (53-34-01A)
- 1995-02-03: SMU - INFO. ON INSPECTION/ MAINTENANCE (I/M) EMISSIONS (51-65-02)
- 1995-02-01: WARRANTY ADMINISTRATION CHEV. CLAIM PROCESSING (42-05-15A)
- 1994-10-25: REV. TO ADHESIVE CAULKING KIT, NEW PRIMERS & PART NUMBERS (43-10-48)
- 1994-09-15: DLR. PRODUCT CAMPAIGN BULLETIN NUMBERING SYSTEM (41-01-03)
- 1994-09-12: INFO. ON NEW PROM/MEMCAL IDENTIFICATION MARKINGS (44-65-01)
- 1994-09-08: CONTAMINATED A/C REFRIGERANT (INFORMATIONAL) (43-12-23)
- 1994-09-01: INFORMATION ANNOUNCING THE NEW CORPORATE BULLETIN (33-01-05A)
- 1994-08-16: OBTAINING TECHNICAL ASSISTANCE (I/M 240 REPAIRS) (43-65-06)
- 1994-07-18: INFORMATION ON RELEASE OF SERVICE PKG. FOR NICKEL TAPE (14-93-01)
- 1994-05-13: WARRANTY ADMINISTRATION - EMISSION WARR. PARTS COVERAGE (47-05-01)
- 1994-04-26: WARRANTY ADMININSTRATION - CLAIM PROCESS CHANGES (42-05-05)
- 1994-04-08: REDUCED PWR STEERING ASSIST AT LOW AMBIENT TEMPERATURES (03-32-06)
- 1994-03-29: ENHANCED INSPECTION MAINTENANCE PROGRAMS (43-65-05)
- 1994-02-15: INFORMATION ON TRANSAXLE OIL FILTER DIFFERENCES (47-71-03)
- 1994-02-01: INFORMATION ON AFTER MARKET ANTI-LOCK BRAKE SYS. PRODUCTS (43-50-01)
- 1993-12-22: RETROFITTING R-12 VEHICLES TO R-134A (INFORMATIONAL) (33-12-26)
- 1993-12-21: SMU - SEC. 3C - FRT. SUSPEN. SPECIFICATION REVISIONS (33-33-03)
- 1993-08-01: INFO. ON COSMETIC DAMAGE TO ALUMINUM WHEELS DURING BALANC. (93-197B-3E)
- 1993-05-25: RECYCLING OF USED OIL FILTERS (INFORMATIONAL) (93-227-0B)
- 1993-05-19: INFO. ON SERVICING VEHICLE WITH CONTAMINATED TRANS. FLUID (93-223-7A)
- 1993-05-19: INFO. ON SERVICING VEHICLE WITH CONTAMINATED TRANS. FLUID (93-7A-142)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (93-201-1A)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (93-1B-126)
- 1993-04-30: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (93-10-194)
- 1993-04-28: SERVICE MANUAL UPDATE STICKERS (93-183-0A)
- 1993-03-16: ILLUSTRATED STEERING SYSTEM BLEED PROCEDURE (38-30-01A)
- 1993-02-01: INDUSTRIAL FALLOUT/RAIL DUST DAMAGE TO BASE COAT/CLEAR COAT (93-58A-10)
- 1993-01-27: INFO. ON FACTORS THAT AFFECT FUEL ECONOMY (30-65-02)
- 1992-12-01: ENG. MISS, HESITATION & ROUGH PIERCED SECONDARY IGNITION (93-6D-102)
- 1992-11-30: SERVICE GUILD: INFO. ON THE EFFECT OF FUEL VOLATILITY (93-6C-100)
- 1992-11-30: ALTERNATE REFRIGERANTS INFORMATION (93-1B-102)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (92-2-128)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-179)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-148)
- 1992-10-31: A/C COMPRESSOR SHAFT NUT REMOVAL (IMPROVED QUALITY) (93-1D-100)
- 1992-10-16: SCUFF/SCRATCH REMOVAL PROCESS ALUM. WHEEL WITH CLEAR COAT (93-20-3E)
- 1992-10-16: SCUFF/SCRATCH REMOVAL PROCESS ALUM. WHEEL WITH CLEAR COAT (93-10-119)
- 1992-10-01: ENG. MISS, HESITATION & ROUGH PIERCED SEC. IGN. COMPONENTS (93-35-6D)
- 1992-10-01: INFO EFFECT FUEL VOLATILITY (DRIVEABILITY CONDITIONS) (93-31-6C)
- 1992-08-03: ALTERNATE REFRIGERANTS INFORMATION (92-250-1A)
- 1992-06-16: SERVICE GUILD: INFO ON AVOID DAMAGE TO TIRE WHEELS (92-232-3E)
- 1992-06-16: SERVICE GUILD: INFO ON AVOID DAMAGE TO TIRE WHEELS (92-3-123)
- 1992-05-31: BRAKE PULSATION SERVICE INFORMATION (88-5-121)
- 1992-05-27: A/C LEAK (DIAGNOSIS BULLETIN) ALL MODELS 1992 AND PRIOR (92-215-1A)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-147-3E)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-3-121)
- 1992-03-20: HARSH SHIFT CONDITIONS AND ON CAR SERVICE INFORMATION (92-130-7A)
- 1992-01-23: SERVICE REPLACEMENT TRANSAXLE (SRTA MODEL UPDATE 4T60-4T60E) (92-86-7A)
- 1992-01-23: SERVICE REPLACEMENT TRANSAXLE (SRTA MODEL UPDATE 4T60-4T60E) (92-74T60-104)
- 1991-12-20: TIRE COMPANY WARRANTY ASSISTANCE PROGRAM (92-70-3E)
- 1991-12-19: AC-DELCO ADVANCE EXCHANGE PGM. PHONE NUMBER CHANGE (92-97-8C)
- 1991-12-18: NEW BOTTOM PAN/CONTROLLED COMP PAN GASKET AND SERVICE INFO. (92-91-7A)
- 1991-12-18: NEW BOTTOM PAN/CONTROLLED COMP PAN GASKET AND SERVICE INFO. (92-74T60-103)
- 1991-11-07: INTERMIT TRANS DOWNSHIFT/SLIP DIAGNOSIS (92-42-7A)
- 1991-11-07: INTERMIT TRANS DOWNSHIFT/SLIP DIAGNOSIS (92-73L80-100)
- 1991-10-11: SELF-ADJUSTER IN REAR CALIPERS NOT FUNCTIONING PROPERLY (88-450-5)
- 1991-09-30: 3-4 CLUTCH/2-4 BAND SERVICE INFORMATION/SERVICE PROCEDURES (91-7-113)
- 1991-08-23: NEW END PLAY SPEC. 4T60/4T60-E (INPUT CARRIER PINION GEAR) (92-11-7A)
- 1991-08-23: NEW END PLAY SPEC. 4T60/4T60-E (INPUT CARRIER PINION GEAR) (92-74T60-100)
- 1991-08-14: SERVICE GUILD: COOLANT RECYCLING UPDATE (91-0-106)
- 1991-08-09: SERVICE GUILD: DETECTING ELECT INTERMITTENTS DIAGNOSTIC (92-05-8A)
- 1991-08-09: SERVICE GUILD: DETECTING ELECT INTERMITTENTS DIAGNOSTIC (92-8-102)
- 1991-08-08: SERVICE GUILD: EVALUATING PEENED SPACER PLATE (91-396-7A)
- 1991-08-08: SERVICE GUILD: EVALUATING PEENED SPACER PLATE (91-7-115)
- 1991-07-26: AC DELCO ADVANCE EXCHANGE PROGRAMS (REVIEW) (91-388-0A)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (91-384-6E)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (91-6-121)
- 1991-06-13: RETAINING MEMORIES IN ELECT. DEVICES WITH BAT. DISCONNECTED (91-8-212)
- 1991-06-11: INFORMATION ON STATE EMISSION TESTING FOR ALL MODELS (91-344-6E)
- 1991-06-11: INFORMATION ON STATE EMISSION TESTING FOR ALL MODELS (91-6-120)
- 1991-05-15: BINDING OR INOP REVERSE STUCK 3-4 SEQ. VALVE 2-3 SHIFT (91-74L60-104)
- 1991-05-10: SERVICE GUILD: HIGH VOL.-LOW PRESSURE PAINT APPLICATION (91-334-10)
- 1991-05-10: SERVICE GUILD: HIGH VOL.-LOW PRESSURE PAINT APPLICATION (91-2-206)
- 1991-04-30: A/C REFRIGERANT LOSS DUE TO LOOSE/MISS. ACCESS FITTING CAP (91-1-123)
- 1991-04-22: EXCESS PAINT IN FLYWHEEL MOUNT HOLES (GOODWRENCH MOTOR 2.5L) (86-273-6)
- 1991-04-22: EXCESS PAINT IN FLYWHEEL MOUNT HOLES (GOODWRENCH MOTOR 2.5L) (91-625-105)
- 1991-04-15: CLEANING OF UPPER I/P SURFACES CLEANING PROCEDURES (91-285-0A)
- 1991-04-15: CLEANING OF UPPER I/P SURFACES CLEANING PROCEDURES (91-2-197)
- 1991-03-12: PAINT ETCHING/STAINING AND PERMANENT WATER SPOTTING (91-251-0B)
- 1991-03-12: PAINT ETCHING/STAINING AND PERMANENT WATER SPOTTING (91-2-175)
- 1991-03-12: CHECKING CLEAR COAT THICKNESS BEFORE & AFTER PAINT FINESSE (91-2-181)
- 1991-02-20: SERVICE MANUAL UPDATE SEC. 10 UNDER BODY DIMENSION CHANGE (90-405-10)
- 1991-02-20: SERVICE MANUAL UPDATE SEC. 10 UNDER BODY DIMENSION CHANGE (91-2-163)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (91-213-6D)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (91-8-172)
- 1991-01-23: NEW DEPARTURE HYATT ROLLER CLUTCH ALL HYDRA-MATIC 3T40 (91-184-7A)
- 1991-01-23: NEW DEPARTURE HYATT ROLLER CLUTCH ALL HYDRA-MATIC 3T40 (91-73T40-103)
- 1991-01-15: SERVICE MAN. UPDATE SEC. 6 NEW ROD BEARING CLEARANCE (91-638-104)
- 1991-01-15: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-73T40-101)
- 1991-01-15: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-74T60105)
- 1991-01-15: NEW 1-2 AND REVERSE BANDS NO SELECTIVE BAND APPLY PINS (91-120-7A)
- 1990-12-31: CHATTERING WIPER BLADES OR WIPEABILITY (91-126-8E)
- 1990-12-31: NO 3RD GEAR AND/OR NO DRIVE OR REVERSE (90-74T60123)
- 1990-12-31: CHATTERING WIPER BLADES OR WIPEABILITY (91-2-123)
- 1990-12-31: BRAKE EFFECTIVENESS AFTER ROTOR REFINISHING (91-5-109)
- 1990-12-31: CHANGE IN BRAKE EFFECTIVENESS AFTER BRAKE WORK (91-133-5)
- 1990-12-15: NEW PLATES-4TH CLUTCH REACTION FORWARD CLUTCH/LOW & REV. (90-74T60-122)
- 1990-12-15: GRINDING OR GROWLING NOISE IN PARK ON INCLINE (90-74T60121)
- 1990-11-27: NEW THERMO ELEMENT & PIN HEIGHT SETTING PROCEDURE (91-142-7A)
- 1990-11-27: NEW THERMO ELEMENT & PIN HEIGHT SETTING PROCEDURE (91-74T60-114)
- 1990-10-16: GASKET IN PLACE OF RTV ON ROCKER ARM COVER (91-102-6)
- 1990-10-16: GASKET IN PLACE OF RTV ON ROCKER ARM COVER (91-625-101)
- 1990-10-09: DRIVE LINK NOISE-IN PARK/ NEUTRAL (91-95-7A)
- 1990-10-09: DRIVE LINK NOISE-IN PARK/ NEUTRAL (91-74T60-108)
- 1990-10-08: NO 3RD GEAR AND/OR NO DRIVE OR REVERSE (91-87-7A)
- 1990-10-08: NO 3RD GEAR AND/OR NO DRIVE OR REVERSE (91-74T60-109)
- 1990-09-21: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-82-7A)
- 1990-09-21: NEW FORWARD CLUTCH LO & REV. WAVED PLATES (91-84-7A)
- 1990-09-21: CHECKING CONNECTOR TERMINAL CONTACT - METRI - PACK (91-85-8A)
- 1990-09-21: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (90-73T40110)
- 1990-09-21: NEW FORWARD CLUTCH LO & REV. WAVED PLATES (91-74T60-106)
- 1990-09-21: CHECKING CONNECTOR TERMINAL CONTACT - METRI - PACK (91-8-108)
- 1990-09-13: NEW SILICONE BEADED SIDE COVER & BOTTOM PAN GASKET (91-71-7A)
- 1990-09-13: NEW SILICONE BEADED SIDE COVER & BOTTOM PAN GASKET (91-73T40-100)
- 1990-08-31: (SRTA) MODEL UPDATE W/3T340 (125C) (91-38-7A)
- 1990-08-24: NEW INPUT INNER SEAL 440-T4 SHORTLIP & 3RD CLUTCH DESIGN (91-53-7A)
- 1990-08-24: NEW INPUT INNER SEAL 440-T4 SHORTLIP & 3RD CLUTCH DESIGN (91-74T60-100)
- 1990-08-14: NEW 1-2 & REVERSE BANDS 440-T4 F7/NO SELECTIVE BAND APPLY PIN (91-74T60-101)
- 1990-06-29: COATED WHEEL WEIGHTS FOR ALUMINUM WHEELS (91-35-3E)
- 1990-06-29: COATED WHEEL WEIGHTS FOR ALUMINUM WHEELS (90-3-127)
- 1990-06-22: BRAKE ROTOR REFINISH PARTS ORDERING INFORMATION (90-293-5)
- 1990-06-22: BRAKE ROTOR REFINISH PARTS ORDERING INFORMATION (90-5-118)
- 1990-06-11: COOLING FAN RUNS BATTERY DEAD (DIAGNOSTIC PROCEDURE) (90-239-6B)
- 1990-05-02: SERVICE REPLACEMENT TRANS. (SRTA) ASSEMBLY MODEL UPDATE (90-7440-117)
- 1990-04-30: HARSH ENGAGE, DOUBLE BUMP OR SHUDDER-PARK/NEUTRAL-REVERSE (90-243-7A)
- 1990-04-30: HARSH ENGAGE, DOUBLE BUMP OR SHUDDER-PARK/NEUTRAL-REVERSE (90-7440-119)
- 1990-04-11: DISTRESSED SECOND CLUTCH 440-T4/4T60 DIAGNOSIS (90-219-7A)
- 1990-04-11: INSTALLATION GUIDELINES FOR AFTERMARKET ACCESSORIES (91-10-8A)
- 1990-04-11: DISTRESSED SECOND CLUTCH 440-T4/4T60 DIAGNOSIS (90-7440-114)
- 1990-04-11: INSTALLATION GUIDELINES FOR AFTERMARKET ACCESSORIES (90-8-184)
- 1990-04-06: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE TESTING (91-09-0A)
- 1990-04-06: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE TESTING (90-6-107)
- 1990-04-06: COOLING FAN RUNS BATTERY DEAD (DIAGNOSTIC PROCEDURE) (90-8-181)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (91-14-8A)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (90-8-170)
- 1990-03-16: NEW 1-2 BAND ASSY. DOES NOT REQUIRE 1-2 BAND STOP (90-197-7A)
- 1990-03-16: NEW 1-2 BAND ASSY. DOES NOT REQUIRE 1-2 BAND STOP (90-7440-112)
- 1990-03-15: MANUAL UPDATE-SEC. 6E1/6E2/6E3 CODE 33,34,63,64 (NON-TURBOS) (90-199-6E)
- 1990-03-15: MANUAL UPDATE-SEC. 6E1/6E2/6E3 CODE 33,34,63,64 (NON-TURBOS) (90-6-105)
- 1990-02-15: INTERMITTENT DELAYED UPSHIFTS HOT OR COLD/PARTS AVAILABLE (90-182-7A)
- 1990-02-15: INTERMITTENT DELAYED UPSHIFTS HOT OR COLD/PARTS AVAILABLE (90-7440-111)
- 1990-01-09: HARSH SHIFT CONDITIONS AND ON CAR SERVICE INFORMATION (90-7440-109)
- 1989-11-09: LOOSE CARPET ON SIDE WALL TRIM PADS (REPAIR PROCEDURE) (90-92-10)
- 1989-11-09: LOOSE CARPET ON SIDE WALL TRIM PADS (REPAIR PROCEDURE) (90-2-114)
- 1989-11-01: REVISED DRIVE LINK WEAR SPECIFICATION 125C - 440T4 (90-191-7A)
- 1989-11-01: REVISED DRIVE LINK WEAR SPECIFICATION 125C - 440T4 (90-7440-104)
- 1989-10-17: SLIPS IN 1ST AND/OR NO 1ST GEAR/NEW PISTON SEALS (89-277-7A)
- 1989-10-17: LTG REQUEST FOR REVIEW UPDATES JULY THRU OCT. 1989 (90-127-0A)
- 1989-10-17: SLIPS IN 1ST AND/OR NO 1ST GEAR/NEW PISTON SEALS (89-7125-116)
- 1989-10-09: RADIO TELEPHONE/MOBILE RADIO INSTALLATION GUIDELINES (90-8-114)
- 1989-09-27: SERVICE GUILD: USE OF FUEL WITH 15% MTBE IN ALL GM VEH. (89-268-0B)
- 1989-09-23: SERVICING CAM AND/OR CRANK GEARS (REPLACE GEAR SET) (89-625-102)
- 1989-09-18: USE GASKET FOR ROCKER ARM COVER INSTEAD OF RTV (90-625-101)
- 1989-09-15: PACKARD CONNECTOR I.D. FOR ALL ECM'S WITH 32 WAY CONNECTORS (90-56-8)
- 1989-09-15: PACKARD CONNECTOR I.D. FOR ALL ECM'S WITH 32 WAY CONNECTORS (90-8-103)
- 1989-08-18: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE INFORMATION (90-49-6B)
- 1989-08-18: THM 440-T4/HYDRA-MATIC 4T60 REPAIR GUIDELINES (90-74-7A)
- 1989-08-18: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE INFORMATION (90-0-101)
- 1989-08-18: THM 440-T4/HYDRA-MATIC 4T60 REPAIR GUIDELINES (90-7440-101)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (89-253-1B)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (89-1-126)
- 1989-07-16: LTG REQUEST FOR REVIEW UPDATES 1989 FEB. THRU JUNE 1989 (90-34-0A)
- 1989-06-20: BROKEN CYLINDER HEAD BOLT COOLANT LOSS (NEW BOLT/GASKET) (87-306-6A)
- 1989-06-20: BROKEN CYLINDER HEAD BOLT COOLANT LOSS (NEW BOLT/GASKET) (89-625-111)
- 1989-06-16: SERVICING CAM AND/OR CRANK GEARS (REPLACE GEAR SET) (90-158-6A)
- 1989-06-16: SERVICING CAM AND/OR CRANK GEARS (REPLACE GEAR SET) (90-625-104)
- 1989-05-29: SPECIAL POLICY: TEMPORARY REDUCTION/POWER STRG.-COLD (88-417-3B)
- 1989-05-29: SPECIAL POLICY: TEMPORARY REDUCTION/POWER STRG.-COLD (9S02)
- 1989-05-24: NEW PROCEDURE FOR REPLACEMENT OF FINAL DRIVE PINION (89-185-7A)
- 1989-05-24: NEW PROCEDURE FOR REPLACEMENT OF FINAL DRIVE PINION (89-7-109)
- 1989-05-23: INTERMITTENT LOSS OF DRIVE CHECK 1-2 BAND STOP (90-17-7A)
- 1989-05-23: TRANSAXLE FINAL DRIVE RATIO -440-T4/4T60 (89-7440-108)
- 1989-05-23: INTERMITTENT LOSS OF DRIVE CHECK 1-2 BAND STOP (89-7440-110)
- 1989-05-18: CHIPPED PAINT DIAGNOSIS AND REPAIR (89-171-10)
- 1989-05-18: CHIPPED PAINT DIAGNOSIS AND REPAIR (89-2-161)
- 1989-05-12: OIL FILTER LEAKAGE PROPER INSTALLATION PROCEDURE (90-216-6)
- 1989-05-12: OIL FILTER LEAKAGE PROPER INSTALLATION PROCEDURE (89-6-115)
- 1989-05-05: POSSIBLE INOP. TORQUE CONV. OR RELATED CONDITION (87-304-7A)
- 1989-05-05: REVISE CODE 35/CHT C-2 IAC CHT ALL 82-89 W/IAC SYSTEM (89-177-6E)
- 1989-05-05: REVISE CODE 35/CHT C-2 IAC CHT ALL 82-89 W/IAC SYSTEM (89-6-112)
- 1989-05-05: POSSIBLE INOP. TORQUE CONV. OR RELATED CONDITION (89-7-108)
- 1989-04-19: SERVICE GUILD: CORRECT CABLE INSULATION FOR CABLE (WIRING) (89-152-8B)
- 1989-04-19: POWER RACK & PINION GEAR SERVICE INFORMATION (89-153-3B)
- 1989-04-19: SERVICE GUILD: CORRECT CABLE INSULATION FOR CABLE (WIRING) (89-8-162)
- 1989-04-18: DIAGNOSIS INFO ON THM 125C LO-REVERSE CLUTCH (89-154-7A)
- 1989-04-18: DIAGNOSIS INFO ON THM 125C LO-REVERSE CLUTCH (89-7125-109)
- 1989-04-14: GOODWRENCH VEHICLE SECURITY SYSTEM LABOR OPERATIONS (89-146-0A)
- 1989-03-31: LIGHT BRAKE DRAG-may BE BRAKE SWITCH ADJUSTMENT (89-262-5)
- 1989-03-31: LIGHT BRAKE DRAG-may BE BRAKE SWITCH ADJUSTMENT (89-5-116)
- 1989-03-02: NO 3RD GEAR (NEW THRUST BEARING) (89-134-7A)
- 1989-03-02: NO 3RD GEAR (NEW THRUST BEARING) (89-7440-106)
- 1989-02-09: A/C REFRIGERANT LOSS DUE TO LOOSE/ MISSING ACCESS FIT. CAP (89-127-1B)
- 1989-02-09: A/C REFRIGERANT LOSS DUE TO LOOSE/ MISSING ACCESS FIT. CAP (89-1-112)
- 1989-02-03: THM 400/475 PRODUCT UPDATE BOOK (89-7400-104)
- 1989-02-01: LABOR TIME GUIDE REQUEST FOR REVIEW CHANGES-sepT/JAN (89-90-0A)
- 1989-01-31: POOR AM OR FM RADIO RECEPTION ANT. COAX. FEMALE TERM. REPAIR (89-108-9A)
- 1989-01-31: POOR AM OR FM RADIO RECEPTION ANT. COAX. FEMALE TERM. REPAIR (89-8-137)
- 1989-01-30: AXLE SEAL PROTECTOR TO PREVENT SEAL DAMAGE DURING INSTALL (89-96-7A-7B)
- 1989-01-30: AXLE SEAL PROTECTOR TO PREVENT SEAL DAMAGE DURING INSTALL (89-7-105)
- 1989-01-18: SERVICE GUILD: ON-CAR BRAKE ROTOR TURNING TOOL (89-85-5)
- 1989-01-18: SERVICE GUILD: ON-CAR BRAKE ROTOR TURNING TOOL (89-5-107)
- 1989-01-10: CAST ALUMINUM WHEEL POROSITY (REPAIR PROC. & SEALER) (89-3-105)
- 1989-01-05: HARSH SHIFT CONDITIONS AND CAR SERVICE INFORMATION (89-7440-105)
- 1988-12-26: SERVICE GUILD: FUEL PUMP STRAINER IN-TANK FILTER/SOCK (89-112-6C)
- 1988-12-26: SERVICE GUILD: FUEL PUMP STRAINER IN-TANK FILTER/SOCK (88-6-125)
- 1988-12-14: LONGER BRAKE PEDAL TRAVEL DIAGNOSIS AND REPAIR (86-265-5)
- 1988-12-14: LONGER BRAKE PEDAL TRAVEL DIAGNOSIS AND REPAIR (88-5-138)
- 1988-11-02: FUEL FEED AND/OR RETURN PIPE REPAIR PROCEDURES (89-31-6C)
- 1988-11-02: FUEL FEED AND/OR RETURN PIPE REPAIR PROCEDURES (89-6-101)
- 1988-10-19: V5 AIR CONDITIONING AND REFRIGERANT SYSTEM DIAGNOSTICS (89-38-1B)
- 1988-10-19: V5 AIR CONDITIONING AND REFRIGERANT SYSTEM DIAGNOSTICS (89-1-110)
- 1988-10-10: BRAKE PULSATION REPLACE SLIDE PINS (88-356-5)
- 1988-10-10: BRAKE PULSATION REPLACE SLIDE PINS (88-5-137)
- 1988-10-07: BRAKE LEAD DIAGNOSIS INFORMATION (89-44-5)
- 1988-10-07: BRAKE LEAD DIAGNOSIS INFORMATION (89-5-101)
- 1988-09-20: NEUTRAL/DRIVE TRANSMISSION GEAR RATTLE INFORMATION (88-351-7B)
- 1988-09-20: NEUTRAL/DRIVE TRANSMISSION GEAR RATTLE INFORMATION (88-7-110)
- 1988-09-19: ELECTRIC FUEL PUMP NOISE DIAGNOSIS AND NEW PARTS (88-638-113)
- 1988-09-01: SERVICE GUILD: A/C COMPRESSOR LINES REVERSED DURING SERVICE (88-370-1B)
- 1988-09-01: SERVICE GUILD: A/C COMPRESSOR LINES REVERSED DURING SERVICE (88-1-147)
- 1988-08-26: DISC BRAKE NOISE GUIDELINES/DESCRIPTIONS (88-340-5)
- 1988-08-26: 1-2 SHIFT SHUDDER - INSTALL NEW FIBER/STEEL CLUTCH PLATE (87-112-7A)
- 1988-08-26: 1-2 SHIFT SHUDDER - INSTALL NEW FIBER/STEEL CLUTCH PLATE (87-7440-108)
- 1988-08-26: DISC BRAKE NOISE GUIDELINES/DESCRIPTIONS (88-5-125)
- 1988-08-22: SERVICE GUILD: THE IMPORTANCE OF FOUR WHEEL ALIGNMENT/ALL (89-01-3A)
- 1988-08-08: ELECTROSTATIC DISCHARGE DAMAGE TO ECM (INFO. TO PREVENT) (88-8-168)
- 1988-08-03: BENCH TYPE SEAT ADJUSTER BINDS REPAIR PROCEDURE (88-321-10)
- 1988-08-03: BENCH TYPE SEAT ADJUSTER BINDS REPAIR PROCEDURE (88-2-214)
- 1988-07-18: SERVICE REPLACEMENT TRANSMISSION ASSEMBLY UPDATE (88-7-108)
- 1988-06-24: ELECTROSTATIC DISCHARGE DAMAGE TO ECM (INFO.TO PREVENT) (88-283-6E)
- 1988-06-24: ELECTROSTATIC DISCHARGE DAMAGE TO ECM (INFO.TO PREVENT) (88-6-118)
- 1988-06-06: SERVICE MANUAL UPDATE UNSTABLE OR INCORRECT IDLE (88-269-6E)
- 1988-06-06: SERVICE MANUAL UPDATE UNSTABLE OR INCORRECT IDLE (88-6-117)
- 1988-05-31: SERVICE MANUAL UPDATE-REVISED CAM GEAR REPLACEMENT PROCEDURE (88-278-6A)
- 1988-05-31: TORQUE STEER -FRT. WHEEL DRIVE DIAGNOSTIC AIDS & PROCEDURE (88-363-3B)
- 1988-05-31: TORQUE STEER -FRT. WHEEL DRIVE DIAGNOSTIC AIDS & PROCEDURE (88-3-130)
- 1988-05-31: SERVICE MANUAL UPDATE-REVISED CAM GEAR REPLACEMENT PROCEDURE (88-625-114)
- 1988-05-19: CLEANING OF UPPER INSTRUMENT PANEL SURFACES (88-242-10)
- 1988-05-19: SERVICE GUILD: INSTALLATION OF AFTER MARKET STYLED WHEELS (88-246-3E)
- 1988-05-19: CLEANING OF UPPER INSTRUMENT PANEL SURFACES (88-2-183)
- 1988-05-17: IDENTIFYING RACK AND PINION STEERING SYSTEM NOISES (88-253-3B)
- 1988-05-17: IDENTIFYING RACK AND PINION STEERING SYSTEM NOISES (88-3-128)
- 1988-05-12: ENGINE COOLING SYSTEM LEAKS (DIAGNOSIS INFORMATION) (88-245-6B)
- 1988-05-12: ENGINE COOLING SYSTEM LEAKS (DIAGNOSIS INFORMATION) (88-6-115)
- 1988-04-25: SPORADIC ENGAGEMENT OF THE TORQUE CONVERTER CLUTCH (88-207-7A)
- 1988-04-25: SPORADIC ENGAGEMENT OF THE TORQUE CONVERTER CLUTCH (88-7-105)
- 1988-04-22: GASOLINE ADDITIVE EXHAUST VALVE RECESSION (86-260-0A)
- 1988-04-22: GASOLINE ADDITIVE EXHAUST VALVE RECESSION (88-6-112)
- 1988-04-04: THM 440-T4 UPDATE BOOK SUMMARIZES PRODUCT CHANGES (88-7440-105)
- 1988-03-15: TCC ENGAGES IN 2ND CHECK TCC SCREEN SEAL P/N (88-201-7A)
- 1988-03-15: TCC ENGAGES IN 2ND CHECK TCC SCREEN SEAL P/N (88-7440-108)
- 1988-03-01: NEW BOTTOM PAN AND COATING CELLULOSE GASKET (88-171-7A)
- 1988-03-01: NEW BOTTOM PAN AND COATING CELLULOSE GASKET (88-7440-106)
- 1988-02-29: SERVICE MANUAL UPDATE THERMAL ELEMENT ON CAR SERVICE (88-163-7A)
- 1988-02-29: ENG. MISS,HESITATION & ROUGH PIERCED SEC. IGN. COMPONENTS (88-6-106)
- 1988-02-29: SERVICE MANUAL UPDATE THERMAL ELEMENT ON CAR SERVICE (88-7440-104)
- 1988-02-22: ERRATIC OR NO UPSHIFT NEW GOVERNOR DRIVEN GEAR (88-161-7A)
- 1988-02-22: ERRATIC OR NO UPSHIFT NEW GOVERNOR DRIVEN GEAR (88-7400-101)
- 1988-02-19: NIBRON COATED INPUT CARRIER THRUST WASHERS W/125-125C (88-156-7A)
- 1988-02-19: NIBRON COATED INPUT CARRIER THRUST WASHERS W/125-125C (88-7125-104)
- 1988-02-01: ENG. MISS, HESITATION & ROUGH PIERCED SEC. IGN. COMPONENTS (88-138-6D)
- 1988-01-25: ENG. STALL WHEN SHIFT TO REV. OR DRIVE AFTER RESTART (87-7125-103)
- 1988-01-25: CORRECT OIL PRESSURE READING DIAGNOSIS AND SWITCH P/N (88-8-119)
- 1988-01-15: TAILGATE POWER LOCK WILL NOT FULLY OPEN DOOR- WAGON (88-125-10)
- 1988-01-15: TAILGATE POWER LOCK WILL NOT FULLY OPEN DOOR- WAGON (88-2-131)
- 1988-01-13: CAMSHAFT LOBE LIFT SPECIFICATIONS (CORRECTION) (88-130-6A)
- 1988-01-13: CAMSHAFT LOBE LIFT SPECIFICATIONS (CORRECTION) (88-625-103)
- 1988-01-11: REMOVAL OF CHEMICAL SPOTTING AND MINOR PAINT IMPERFECTIONS (88-135-10)
- 1988-01-08: MANUAL SEAT BACK RECLINER COMMENTS (87-262-10)
- 1988-01-08: MANUAL SEAT BACK RECLINER COMMENTS (87-2-252)
- 1988-01-04: NEW DESIGN FUEL SYS. PULSATOR REDUCE FUEL PUMP NOISE (87-628-123)
- 1988-01-04: NEW DESIGN FUEL SYS. PULSATOR REDUCE FUEL PUMP NOISE (87-630-108)
- 1988-01-04: NEW DESIGN FUEL SYS. PULSATOR REDUCE FUEL PUMP NOISE (87-638-113)
- 1988-01-01: ENG. STALL WHEN SHIFT TO REV. OR DRIVE AFTER RESTART (87-260-7A)
- 1987-12-28: FUEL PUMP NOISE ON COUPES & SEDANS WITH V-6 ENGINE (87-142)
- 1987-12-28: FUEL PUMP NOISE ON COUPES & SEDANS WITH V-6 ENGINE (87-628-111)
- 1987-12-28: FUEL PUMP NOISE ON COUPES & SEDANS WITH V-6 ENGINE (87-630-103)
- 1987-12-28: FUEL PUMP NOISE ON COUPES & SEDANS WITH V-6 ENGINE (87-638-108)
- 1987-12-21: CORRECT OIL PRESSURE READING DIAGNOSIS AND SWITCH P/N (88-114-6)
- 1987-12-21: CORRECT OIL PRESSURE READING DIAGNOSIS AND SWITCH P/N (88-628-109)
- 1987-12-15: TRANSMISSION VALVE BODY COVER/OIL PAN LEAKS (88-118-7A)
- 1987-12-15: TRANSMISSION VALVE BODY COVER/OIL PAN LEAKS (88-7125-100)
- 1987-12-11: NEW DESIGN INPUT CLUTCH AND THIRD CLUTCH SEAL INSTALLERS (88-119-7A)
- 1987-12-11: NEW DESIGN INPUT CLUTCH AND THIRD CLUTCH SEAL INSTALLERS (88-7440-102)
- 1987-12-08: NEW DESIGN SECOND CLUTCH PISTON INNER SEAL (88-111-7A)
- 1987-12-08: NEW DESIGN SECOND CLUTCH PISTON INNER SEAL (88-7440-101)
- 1987-12-01: DAMAGE TO WIRING TERMINALS ON ENGINE SENSORS-METRI-PACK 150 (88-101-8A)
- 1987-12-01: DAMAGE TO WIRING TERMINALS ON ENGINE SENSORS-METRI-PACK 150 (88-8-117)
- 1987-11-16: TIRE WARRANTIES IRREGULAR/PREMATURE WEAR (88-116-3E)
- 1987-11-16: TIRE WARRANTIES IRREGULAR/PREMATURE WEAR (88-3-104)
- 1987-11-10: INTERMITTENT OR NO DRIVE OR REVERSE (MAY BE SPRAG OR RACE) (86-258-7A)
- 1987-11-10: INTERMITTENT OR NO DRIVE OR REVERSE (MAY BE SPRAG OR RACE) (87-7440-105)
- 1987-10-19: INSTRUMENT CLUSTER EXCHANGE PROGRAM INFORMATION (88-8-106)
- 1987-10-09: HARSH 1-2 SHIFT CONDITION CHECK 2ND CLUTCH FEED (87-246-7A)
- 1987-10-09: HARSH 1-2 SHIFT CONDITION CHECK 2ND CLUTCH FEED (87-7440-119)
- 1987-10-07: REAR BRAKE DRUM FREEZE INSTALL NEW BACKING PLATE P/N (87-238-5)
- 1987-10-07: REAR BRAKE DRUM FREEZE INSTALL NEW BACKING PLATE P/N (87-5-117)
- 1987-10-01: DELAYED 2/3 SHIFT/LOSS OF 3RD THM 440-T4 3RD CLUTCH SEAL (87-191)
- 1987-10-01: DELAYED SHIFT THM 440-T4 3RD CLUTCH SEAL (87-70)
- 1987-10-01: DELAYED 2/3 SHIFT/LOSS OF 3RD THM 440-T4 3RD CLUTCH SEAL (87-7440-104)
- 1987-09-28: GLOVE BOX DOOR WARPED OR IMPROPER FIT-REPLACEMENT P/N (87-234-10)
- 1987-09-28: GLOVE BOX DOOR WARPED OR IMPROPER FIT-REPLACEMENT P/N (87-2-216)
- 1987-09-24: RADIAL TIRE/LEAD PULL CORRECTION CHARTS (87-212-3)
- 1987-09-23: TPS SPECIFICATIONS INFORMATION (88-55)
- 1987-09-23: TPS SPECIFICATIONS INFORMATION (88-628-104)
- 1987-09-15: THM 125C SRTA PROGRAM GUIDELINE INFORMATION (86-251)
- 1987-09-15: RATTLE NOISE FROM TURN SIGNAL LEVER (INSTALL FOAM DONUT) (87-224)
- 1987-09-15: RATTLE NOISE FROM TURN SIGNAL LEVER (INSTALL FOAM DONUT) (87-2-215)
- 1987-09-08: TRANSMISSION FLEXPLATE CRACKS 2.8 W/ A/T -REPLACE DOWEL PIN (87-219)
- 1987-09-08: TRANSMISSION FLEXPLATE CRACKS 2.8 W/ A/T -REPLACE DOWEL PIN (87-628-119)
- 1987-09-04: ECM RESET/ FAILURE DIAGNOSIS INFORMATION (87-6-117)
- 1987-08-20: STEERING LEAD OR PULL DIAGNOSIS AND POSSIBLE REPAIR (87-3-132)
- 1987-08-18: FUEL PUMP RUN-ON AFTER ENGINE TURNED OFF (87-210)
- 1987-08-14: SERVICE GUILD: SERVICE REPL. ECM WITH PROM INSTALLED (88-42)
- 1987-08-10: ERRATIC SHIFT/ NO SHIFT SEALER IN GOVERNOR PASSAGES (87-208)
- 1987-08-10: ERRATIC SHIFT/ NO SHIFT SEALER IN GOVERNOR PASSAGES (87-7440-115)
- 1987-08-04: SOFT, SLIPPING/NO 1-2 SHIFT POSSIBLE CLUTCH HSG WEAR (86-246)
- 1987-08-04: SOFT, SLIPPING/NO 1-2 SHIFT POSSIBLE CLUTCH HSG WEAR (87-7440-112)
- 1987-08-03: DELAYED 2/3 SHIFT/LOSS OF 3RD THM 440-T4 3RD CLUTCH SEAL (87-7440-110)
- 1987-08-03: SECOND GEAR STARTS SERVICE ACTION (87-7440-111)
- 1987-07-16: TILT STEERING COLUMN NOISE LUBRICATE LOCK BOLT (87-194)
- 1987-07-16: TILT STEERING COLUMN NOISE LUBRICATE LOCK BOLT (87-3-129)
- 1987-07-01: SECOND GEAR STARTS THM-440-T4 TRANSAXLE (87-179)
- 1987-07-01: ANALYSIS OF ENGINES WITH INTERNAL SLUDGE ACCUMULATION (87-182)
- 1987-06-16: ENGINE FLARE,SLIPS, NO DRIVE ON TURNS - 84-87 THM 440T4 (87-202)
- 1987-06-16: ENGINE FLARE SLIPS NO DRIVE ON TURNS -84-87 THM 440T4 (87-168)
- 1987-06-16: ENGINE FLARE,SLIPS, NO DRIVE ON TURNS - 84-87 THM 440T4 (87-7440-109)
- 1987-06-03: TIRE COMPANY ASSISTANCE PROGRAM (87-158)
- 1987-05-29: GASOLINE MARKETED/ADVERTISED KEEP PORT FUEL INJECTORS CLEAN (87-165)
- 1987-05-28: INTERMITTENT NO REVERSE MUST SHIFT TO DRIVE FIRST (87-160)
- 1987-05-28: INTERMITTENT NO REVERSE MUST SHIFT TO DRIVE FIRST (87-7440-117)
- 1987-05-26: COLD START INJECTOR 'O' RING REPLACEMENT (87-153)
- 1987-05-26: COLD START INJECTOR 'O' RING REPLACEMENT (87-628-113)
- 1987-05-14: NEW ECM TEST PROCEDURES ALL ECM EQUIPPED VEHICLES (87-150)
- 1987-05-14: NEW ECM TEST PROCEDURES ALL ECM EQUIPPED VEHICLES (87-6-115)
- 1987-05-01: HARSH ENGAGEMENT NEUTRAL TO DRIVE OR REVERSE (87-133)
- 1987-05-01: HARSH ENGAGEMENT NEUTRAL TO DRIVE OR REVERSE (87-7125-104)
- 1987-04-30: TIRE /WHEEL VIBRATION EXISTS SPECIAL HANDLING TIRES (87-130)
- 1987-04-30: TIRE /WHEEL VIBRATION EXISTS SPECIAL HANDLING TIRES (87-3-122)
- 1987-04-30: VIBRATION CAUSED BY EXCESSIVE WHEEL RUNOUT (86-3-128)
- 1987-04-10: PARK BRAKE EQUALIZER NOISE INSTALL INSULATOR AS OUTLINED (87-113)
- 1987-04-10: BRAKES BIND/SLOW PEDAL RETURN PUSH ROD & PEDAL ARM BIND (87-117)
- 1987-04-10: ENG. STALL WHEN SHIFT TO REV. OR DRIVE AFTER RESTART (87-111)
- 1987-04-10: BRAKES BIND/SLOW PEDAL RETURN PUSH ROD & PEDAL ARM BIND (87-5-104)
- 1987-04-10: PARK BRAKE EQUALIZER NOISE INSTALL INSULATOR AS OUTLINED (87-5-107)
- 1987-04-07: ENG. MAY INTERMITTENTLY STALL CHECK FOR RESIDUE ON THROTTLE (87-109)
- 1987-04-07: ENG. MAY INTERMITTENTLY STALL CHECK FOR RESIDUE ON THROTTLE (87-628-109)
- 1987-04-07: METHOD OF VERIFYING ' GOOD ELECTRICAL SYSTEM GROUND ' (87-8-139)
- 1987-04-03: SERVICE REPLACEMENT CRANKSHAFT P/N LISTED (87-101)
- 1987-04-03: SERVICE REPLACEMENT CRANKSHAFT P/N LISTED (87-625-107)
- 1987-03-23: FUEL STARVATION W/NOSE PARKED DOWN - 1/4 TANK OF FUEL (87-638-105)
- 1987-03-16: CAST ALUMINUM WHEEL POROSITY REPAIR AND SEALER REVISED (89-59-3E)
- 1987-03-16: CAST ALUMINUM WHEEL POROSITY REPAIR AND SEALER REVISED (87-3-115)
- 1987-03-16: HARD START OR EXTENDED CRANK AFTER HOT OR COLD SOAK (86-227)
- 1987-03-16: HARD START OR EXTENDED CRANK AFTER HOT OR COLD SOAK (86-628-114)
- 1987-02-25: FUEL STARVATION W/NOSE PARKED DOWN - 1/4 TANK FUEL (87-83)
- 1987-02-25: FUEL STARVATION W/NOSE PARKED DOWN - 1/4 TANK FUEL (87-628-105)
- 1987-01-08: TV SYSTEM DIAG.-ALL A/T EXCEPT THM 180,350,400 (87-55)
- 1987-01-08: TV SYSTEM DIAG.-ALL A/T EXCEPT THM 180,350,400 (87-7-101)
- 1987-01-06: BLUSHING EXTERIOR W / DISPERSION LAQUER PAINT (85-129)
- 1987-01-06: BLUSHING EXTERIOR W / DISPERSION LAQUER PAINT (87-2-117)
- 1986-12-15: INTERMEDIATE PIPE REPLACEMENT ON ALL WELDED EXHAUST SYSTEMS (86-6-138)
- 1986-12-15: INSTRUMENT CLUSTER EXCHANGE PROGRAM INFORMATION (87-8-113)
- 1986-12-11: ENGINE SURGE MAY NEED SERVICE PROM (86-212)
- 1986-12-11: ENGINE DETONATION/CHUGGLE MAY NEED SERVICE PROM (86-213)
- 1986-12-11: ENGINE SURGE MAY NEED SERVICE PROM (86-628-112)
- 1986-12-11: ENGINE DETONATION/CHUGGLE MAY NEED SERVICE PROM (86-628-113)
- 1986-12-09: LOOSE W/S WIPER ARMS NEW STYLE WIPER ARMS AVAIL. (86-209)
- 1986-12-09: LOOSE W/S WIPER ARMS NEW STYLE WIPER ARMS AVAIL. (86-2-179)
- 1986-12-01: PORT FUEL INJ. REPLACEMENT USAGE AND P/N'S LISTED (87-36)
- 1986-12-01: PORT FUEL INJ. REPLACEMENT USAGE AND P/N'S LISTED (87-628-104)
- 1986-11-12: REDUCE THROTTLE PEDAL EFFORT ELIMINATE RETURN SPRING (87-27)
- 1986-11-12: REDUCE THROTTLE PEDAL EFFORT ELIMINATE RETURN SPRING (87-7440-101)
- 1986-11-07: VIBRATION DIAGNOSIS 'REED' TACHOMETER INFORMATION (87-139)
- 1986-11-07: CLEAN PORT FUEL INJECTORS GASOLINE ADDITIVES (87-25)
- 1986-11-07: CLEAN PORT FUEL INJECTORS GASOLINE ADDITIVES (87-0-106)
- 1986-11-06: OIL LEAK AT OIL PAN DRAIN PLUG V-8, V6, OHV L4 CARS & TRUCKS (86-118)
- 1986-11-06: OIL LEAK AT OIL PAN DRAIN PLUG V-8, V6, OHV L4 CARS & TRUCKS (86-6-122)
- 1986-10-31: REPETITIVE INOP A/C COMPRESSOR FLUSHING PROCEDURE REVISED (87-21)
- 1986-10-31: REPETITIVE INOP A/C COMPRESSOR FLUSHING PROCEDURE REVISED (87-1-102)
- 1986-10-29: HARSH NEUTRAL TO REVERSE/DRIVE CHECK VACUUM LINE FOR BLOCKAGE (87-190)
- 1986-10-29: HARSH NEUTRAL TO REVERSE/DRIVE CHECK VACUUM LINE FOR BLOCKAGE (87-7440-100)
- 1986-10-20: USE OF UNLEADED GASOLINE IN VEHICLES USING LEADED GAS (87-6-100)
- 1986-10-13: HARSH UPSHIFTS/3-2 SHIFTS SERVICE INFORMATION (440-T4) (86-190R)
- 1986-10-13: REVISED: HARSH UPSHIFTS / 3-2 SERVICE INFORMATION (440-T4) (86-170)
- 1986-10-09: NEW PARTS/ SERVICE INFORMATION 440-T4 TRANSMISSION (86-191)
- 1986-10-09: NEW PARTS/ SERVICE INFORMATION 440-T4 TRANSMISSION (86-7440-109)
- 1986-10-06: HARSH UPSHIFTS AT HIGH ALTITUDES (86-7400-108)
- 1986-09-24: CHATTERING WIPER BLADES CLEAN BLADES/GLASS (84-102)
- 1986-09-24: REVISED:CHATTERING BLADES CLEAN BLADES/GLASS (84-2-140)
- 1986-09-24: CHATTERING WIPER BLADES CLEAN BLADES/GLASS (87-2-106)
- 1986-09-23: COLOR COAT CHIPS OFF GUIDELINES FOR INSPECTION (87-09)
- 1986-09-23: USE OF UNLEADED GASOLINE VEHICLES USING LEADED GAS (87-0-104)
- 1986-09-23: COLOR COAT CHIPS OFF GUIDELINES FOR INSPECTION (87-2-101)
- 1986-09-22: DELCO FREEDOM BATTERY STORAGE AND TESTING (87-8-108)
- 1986-09-15: PAINT/CARE OF CAR FINISHES ALL VEHICLES AFFECTED (87-2-100)
- 1986-09-09: HARD TO PRESS THROTTLE PEDAL SERVICE KIT FOR E2SE CARB. (86-181R)
- 1986-09-09: HARD TO PRESS THROTTLE PEDAL SERVICE KIT FOR E2SE CARB. (86-628-108)
- 1986-09-06: NO UPSHIFT AFTER A PART OR FULL THROTTLE DETENT (86-169)
- 1986-09-06: NO UPSHIFT AFTER A PART OR FULL THROTTLE DETENT (86-7200-103)
- 1986-09-04: A/T OIL COOLER FLUSHING ALL THM A/T MODELS (86-164)
- 1986-09-04: A/T OIL COOLER FLUSHING ALL THM A/T MODELS (87-7-100)
- 1986-09-01: NO UPSHIFT CONDITION AFTER DOWNSHIFT AUTO. TRANSMISSION (86-159)
- 1986-08-28: COLOR SANDING NOT RECOMMENDED BASECOAT/CLEARCOAT VEHICLES (86-168)
- 1986-08-28: SQUEAK NOISE IN STEERING WHEEL LUBRICATE TILT WHEEL ASSEMBLY (87-07)
- 1986-08-28: SERVICE GUILD: ELECTROSTATIC DISCHARGE DAMAGE (87-08)
- 1986-08-28: SQUEAK NOISE IN STEERING WHEEL LUBRICATE TILT WHEEL ASSEMBLY (87-3-100)
- 1986-08-28: SERVICE GUILD: ELECTROSTATIC DISCHARGE DAMAGE (87-8-102)
- 1986-08-20: REVISION-DIAGNOSTIC ROUTING ON SPECMO C/C QUICK CHECKERS (86-157)
- 1986-08-14: REWORK OF REAR COMPARTMENT LID HINGE ASSEMBLY (87-03)
- 1986-08-14: REWORK OF REAR COMPARTMENT LID HINGE ASSEMBLY (87-2-103)
- 1986-08-11: SUMMARY OF SHUDDER THM 440-T4 DIAGNOSIS-POTENTIAL CAUSES (86-155)
- 1986-08-11: INOPERATIVE TPS INSTALL HEAT SHIELD (86-625-110)
- 1986-08-11: SUMMARY OF SHUDDER THM 440-T4 DIAGNOSIS-POTENTIAL CAUSES (86-7440-104)
- 1986-08-01: HIGH SHIFT EFFORT NON-TILT STEERING WHEEL (86-144)
- 1986-08-01: HIGH SHIFT EFFORT NON-TILT STEERING WHEEL (86-7440-107)
- 1986-07-30: OIL PUMP ROTOR AND SLIDE UPDATED P/N'S LISTED 125/125C (86-151)
- 1986-07-30: OIL PUMP ROTOR AND SLIDE UPDATED P/N'S LISTED 125/125C (86-7125-110)
- 1986-07-28: UNLEADED GAS BRANDS PORT FUEL INJECTION (86-147)
- 1986-07-23: DELCO FREEDOM BATTERY DIAGNOSIS-CHARGING INFORMATION (86-187)
- 1986-07-23: DELCO FREEDOM BATTERY DIAGNOSIS-CHARGING INFORMATION (87-8-109)
- 1986-07-21: WIRE WHEEL COVER NOISE INSTALL NYLON CLIPS (85-26)
- 1986-07-21: WIRE WHEEL COVER NOISE INSTALL NYLON CLIPS (84-3-106)
- 1986-07-18: SQUEAK/NOISE DISC BRAKE NEW P/N LINING MATERIAL (86-139)
- 1986-07-18: SQUEAK/NOISE DISC BRAKE NEW P/N LINING MATERIAL (86-5-119)
- 1986-07-15: TRANSMISSION BULLETIN SUMMARY LISTING (86-92)
- 1986-07-15: RACK & PINION POWER STEERING REMANUFACTURED GEARS (86-3-118)
- 1986-07-15: TRANSMISSION BULLETIN SUMMARY LISTING (86-7-105)
- 1986-07-10: FORWARD CLUTCH HOUSING CHANGE CORRECTS HARSH PARK TO DRIVE (84-267)
- 1986-07-10: FORWARD CLUTCH HOUSING CHANGE CORRECTS HARSH PARK TO DRIVE (86-7125-109)
- 1986-07-09: SP. POLICY: REPLACE FLEX VANE WINDSHIELD WASHER PUMP (85-211)
- 1986-07-09: SP. POLICY: REPLACE FLEX VANE WINDSHIELD WASHER PUMP (86-8-146)
- 1986-07-03: CHECK ENGINE LIGHT CODE 34 DIAGNOSIS INFORMATION LISTED (85-202)
- 1986-07-03: CHECK ENGINE LIGHT CODE 34 DIAGNOSIS INFORMATION LISTED (85-6-307)
- 1986-07-02: METHOD OF REMOVING ROCKER ARM COVERS (86-111)
- 1986-07-02: METHOD OF REMOVING ROCKER ARM COVERS (86-625-108)
- 1986-07-01: INOPERATIVE TPS INSTALL HEAT SHIELD (86-122)
- 1986-07-01: V5 A/C COMPRESSOR SERVICEABILITY PART NUMBERS (86-87)
- 1986-07-01: SUPPLEMENT: VARIABLE DISPLACEMENT A/C 'O' RING (86-119)
- 1986-07-01: INOPERATIVE TPS INSTALL HEAT SHIELD (86-618-106)
- 1986-07-01: V5 A/C COMPRESSOR SERVICEABILITY PART NUMBERS (85-1-112)
- 1986-06-20: CLEAR COAT ON ALUMINUM WHEELS REPAIR PROCEDURE OUTLINED (86-131R)
- 1986-06-20: CLEAN, PAINT AND COAT ALL MODELS W/ ALUMINUM WHEELS (84-127)
- 1986-06-20: CLEAN, PAINT & COATING OF ALUMINUM WHEELS (85-3-118)
- 1986-06-20: REVISED:TRUNK LAMP ASSY. DEAD BATTERYNEW P/N (86-8-138)
- 1986-06-16: IRREGULAR/PREMATURE TIRE WEAR REPAIR/ROTATION PROCEDURE (86-90)
- 1986-06-10: REPLACE INTERMEDIATE PIPE WELDED EXHAUST SYSTEMS (86-109)
- 1986-06-10: REPLACE INTERMEDIATE PIPE WELDED EXHAUST SYSTEMS (86-8-134)
- 1986-06-05: DIESEL: GLOW PLUG CONTROL MODULE FAILS (TIMER REPAIR) (85-208)
- 1986-06-05: DIESEL: GLOW PLUG CONTROL MODULE FAILS (TIMER REPAIR) (85-6-313)
- 1986-06-03: HARD TO RELEASE HOOD LATCH CHECK BUMPER AND STRIKER ADJ. (86-103)
- 1986-06-03: HARD TO RELEASE HOOD LATCH CHECK BUMPER AND STRIKER ADJ. (86-2-144)
- 1986-05-30: PREMATURE BRAKE WEAR-BRAKES ENGAGED AFTER PEDAL RELEASED (86-108)
- 1986-05-30: PREMATURE BRAKE WEAR-BRAKES ENGAGED AFTER PEDAL RELEASED (86-5-113)
- 1986-05-19: ENGINE SURGE AFTER HOT SOAK CARB. PRIMARY METERING JETS (86-650-102)
- 1986-05-13: SURGE WHEN TCC ENGAGES NEW PROM P/N TO REVISE TCC (86-100)
- 1986-05-13: SURGE WHEN TCC ENGAGES NEW PROM P/N TO REVISE TCC (86-625-107)
- 1986-05-06: 440T4 TCC OPERATION SERVICE MANUAL UPDATE (86-7440-105)
- 1986-04-10: BUZZ FELT IN ACC. PEDAL NEW SPACER PLATE P/N (86-77)
- 1986-04-10: BUZZ FELT IN ACC. PEDAL NEW SPACER PLATE P/N (86-7125-106)
- 1986-04-09: FLUID LEAK DETECTION SPEC. FLUID/BLACK LIGHT USE (86-83)
- 1986-04-09: BRAKE PULSATIONS DUE TO UNEVEN OR RUSTY ROTOR/BRAKE DRUM (86-84)
- 1986-04-09: FLUID LEAK DETECTION SPEC. FLUID/BLACK LIGHT USE (86-0-108)
- 1986-04-09: BRAKE PULSATIONS DUE TO UNEVEN OR RUSTY ROTOR/BRAKE DRUM (86-5-109)
- 1986-04-04: POPPING NOISE WHEN BRAKING FORE / AFT SHIFT OF FRAME (85-97)
- 1986-04-04: REVISED:POP NOISE WHEN BRAKING FORE / AFT SHIFT OF FRAME (86-69)
- 1986-04-04: POPPING NOISE WHEN BRAKING FORE / AFT SHIFT OF FRAME (86-6-115)
- 1986-03-24: GLOVE BOX DOOR FIT CORRECT ADJUSTMENT (86-67)
- 1986-03-24: METHOD TO REMOVE PUSH ROD COVERS W/O COVER DAMAGE (86-74)
- 1986-03-24: GLOVE BOX DOOR FIT CORRECT ADJUSTMENT (86-2-133)
- 1986-03-24: METHOD TO REMOVE PUSH ROD COVERS W/O COVER DAMAGE (86-625-105)
- 1986-03-20: ROUGH IDLE,SURGE,MISFIRE AND / OR POOR PERFORMANCE (86-64)
- 1986-03-20: ROUGH IDLE,SURGE,MISFIRE AND / OR POOR PERFORMANCE (86-628-101)
- 1986-03-19: ELECTRIC FUEL PUMP HUM NOISE (85-196)
- 1986-03-19: ELECTRIC FUEL PUMP HUM NOISE (85-6-306)
- 1986-03-14: ACCESSORY DRIVE BELT TENSION SHOP MANUAL OMISSION (86-63)
- 1986-03-11: LOOSE WHEEL COVER-SQUEAKS INSTALL NYLON CLIPS (85-193)
- 1986-03-11: LOOSE WHEEL COVER-SQUEAKS INSTALL NYLON CLIPS (85-3-147)
- 1986-03-04: BASECOAT CLEARCOAT EXTERIOR MACH. POLISH NOT RECOMMENDED (86-45)
- 1986-03-04: BASECOAT CLEARCOAT EXTERIOR MACH. POLISH NOT RECOMMENDED (86-2-126)
- 1986-03-01: CAMPAIGN:TORQUE CONVERTER GROUND WIRE REVISION (5R27)
- 1986-03-01: 700-R4 SERVICE REPLACEMENT TRANS. ASSEMBLY (SRTA) PROGRAM (86-7700-100)
- 1986-02-26: CONTROL VALVE ASSEMBLY CLEANING/SERVICING - ALL A/T (86-49)
- 1986-02-26: CONTROL VALVE ASSEMBLY CLEANING/SERVICING - ALL A/T (86-7-103)
- 1986-02-17: HARSH 1-2 AND 2-3 UP SHIFTS THM 400 (VR-VV) (86-7400-100)
- 1986-02-01: ON-VEHICLE CLEANING OF PORT FUEL INJECTORS (86-19)
- 1986-02-01: NO UPDATE AFTER A PART OR FULL THROTTLE DETENT (85-7-170)
- 1986-01-31: HARD/NO START HOT FUEL STARVATION AT HIGH ALTITUDES (85-181)
- 1986-01-31: REMANUFACTURED TBI FUEL INJECTORS (APPLICATION) (86-36)
- 1986-01-31: TRANSAXLE CASE INTERMEDIATE SERVO ORIFICE ELIMINATED (86-40)
- 1986-01-31: HARD/NO START HOT FUEL STARVATION AT HIGH ALTITUDES (85-6-287)
- 1986-01-31: REMANUFACTURED TBI FUEL INJECTORS (APPLICATION) (86-6-129)
- 1986-01-31: TRANSAXLE CASE INTERMEDIATE SERVO ORIFICE ELIMINATED (86-7125-105)
- 1986-01-23: THM 125 OR 125C TRANSAXLE SLIPPING IN ALL RANGES (86-32)
- 1986-01-23: AUTOMATIC TRANSMISSION IDENTIFICATION INFORMATION (86-51)
- 1986-01-23: AUTOMATIC TRANSMISSION IDENTIFICATION INFORMATION (86-7-102)
- 1986-01-23: THM 125 OR 125C TRANSAXLE SLIPPING IN ALL RANGES (86-7125-104)
- 1986-01-23: ROUGH IDLE OR POOR PERFORMANCE (CHECK INTAKE PLENUM RUNNERS) (86-34)
- 1986-01-23: ROUGH IDLE OR POOR PERFORMANCE (CHECK INTAKE PLENUM RUNNERS) (86-628-100)
- 1986-01-22: INTERMITTENT WIPER OPERTION REPLACE END CAP (85-188)
- 1986-01-22: INTERMITTENT WIPER OPERTION REPLACE END CAP (85-8-152)
- 1986-01-10: VIBRATION IN STEERING WHL,FLR, INST PNL, SEAT-ALT. BELT VIB. (85-175)
- 1986-01-10: VIBRATION IN STEERING WHL,FLR, INST PNL, SEAT-ALT. BELT VIB. (85-6-295)
- 1986-01-02: ENGINE OIL DISCOLORATION OIL LEAK DETECTION (86-25)
- 1985-12-23: WORK AREA & EQUIP. REQUIREMENT TO OVERHAUL TRANSMISSIONS (86-7-101)
- 1985-12-05: VISTA VENT HARDWARE NUT W/INTEGRAL SEAL (85-171)
- 1985-12-05: VISTA VENT HARDWARE NUT W/INTEGRAL SEAL (86-2-113)
- 1985-12-02: ALTERNATOR WHINE-LEFT CHANNEL MODIFY GROUND TO RADIO (86-22)
- 1985-12-02: ALTERNATOR WHINE-LEFT CHANNEL MODIFY GROUND TO RADIO (86-8-111)
- 1985-12-01: CORRECTION TO DIAGNOSTIC CHARTS SHOP MANUAL (86-14)
- 1985-11-27: IRREGULAR REAR TIRE WEAR TIRE NOISE / ROUGHNESS (86-23)
- 1985-11-27: IRREGULAR REAR TIRE WEAR TIRE NOISE / ROUGHNESS (86-3-107)
- 1985-11-25: DIAGNOSIS USING ALDL FUEL FLOW ERRORS-INTEGRATOR/BLOCK LEARN (86-8)
- 1985-11-25: DIAGNOSIS USING ALDL FUEL FLOW ERRORS-INTEGRATOR/BLOCK LEARN (86-6-101)
- 1985-11-19: BROKEN ENGINE STRUT BRACKET/ CYLINDER HEAD BRACKET BOLT (85-162)
- 1985-11-19: BROKEN ENGINE STRUT BRACKET/ CYLINDER HEAD BRACKET BOLT (85-7-167)
- 1985-11-18: QUIET TURN SIGNAL FLASHERS HIGHER NOISE LEVEL FLASHER P/N (86-6)
- 1985-11-18: SCAN TOOL WORKSHEET ALL ECM EQUIPPED VEHICLES (85-6-259)
- 1985-11-18: QUIET TURN SIGNAL FLASHERS HIGHER NOISE LEVEL FLASHER P/N (86-8-110)
- 1985-11-13: LUBRICATION OF LOCK CYLINDERS PROPER LUBRICANTS/PRECAUTIONS (86-15)
- 1985-11-13: DELAYED FORWARD ENGAGEMENT SLIPS ON TAKEOFF/2-3 UPSHIFT (86-65)
- 1985-11-13: LUBRICATION OF LOCK CYLINDERS PROPER LUBRICANTS/PRECAUTIONS (86-2-105)
- 1985-11-13: DELAYED FORWARD ENGAGEMENT SLIPS ON TAKEOFF/2-3 UPSHIFT (86-7440-101)
- 1985-11-01: HARD OR NO START AND/OR DOES NOT MAINTAIN FUEL PRESSURE (85-161)
- 1985-11-01: HARD OR NO START AND/OR DOES NOT MAINTAIN FUEL PRESSURE (85-6-268)
- 1985-10-29: RECOMMENDED RTV SEALANTS P/N'S AND APPLICATIONS (86-10)
- 1985-10-25: CAMPAIGN: CLUTCH CABLE NOT PROPERLY SECURED (85-C-19A)
- 1985-10-25: CAMPAIGN: CLUTCH CABLE NOT PROPERLY SECURED (85-C-19)
- 1985-10-23: DA6 A/C COMPRESSOR REPAIR REPAIR ASSEMBLY P/N (85-157)
- 1985-10-23: DA6 A/C COMPRESSOR REPAIR REPAIR ASSEMBLY P/N (86-1-100)
- 1985-10-21: 6000 MANUAL UPDATE PAGE OMITTED FROM MANUAL (85-3-141)
- 1985-10-17: SIX WAY POWER SEAT ADJUSTER IMPROVEMENTS- NEW P/N'S (85-148)
- 1985-10-17: SIX WAY POWER SEAT ADJUSTER IMPROVEMENTS- NEW P/N'S (86-8-103)
- 1985-10-11: DELAYED ENGAGEMENT-CRUISE III MISDIAGNOSED AS MALFUNCTION (85-146)
- 1985-10-11: DELAYED ENGAGEMENT-CRUISE III MISDIAGNOSED AS MALFUNCTION (85-9-113)
- 1985-10-11: NEW POWER DOOR LOCK SWITCH MODULE (85-8-149)
- 1985-10-09: SIMULATED CONVERTIBLE TOP REVISED VINYL REPAIR PROCEDURE (85-149)
- 1985-10-09: SIMULATED CONVERTIBLE TOP REVISED VINYL REPAIR PROCEDURE (85-2-165)
- 1985-10-07: ALUM. WHEEL REFINISHING ALTERNATIVE PROCEDURE (85-3-140)
- 1985-10-07: CRACKED PAINT USING RM HIGH SOLIDS RAPID FILTER (86-2-103)
- 1985-10-02: OIL FILTER CHANGE NOT REQUIRED AS A RESULT OF SPARK PLUG FOUL (86-20)
- 1985-10-02: WHEEL LOCK INFORMATION TWO TYPES OF LOCKS (86-5)
- 1985-10-02: NEW GASKETS: TRANSAXLE OIL PAN AND VALVE BODY COVER (86-76)
- 1985-10-02: NEW TRANSMISSION PAN GASKET ALL THM-125C TRANSMISSIONS (85-130)
- 1985-10-02: REVISED:NEW TRANSAXLE GASKET AND VALVE BODY COVER (86-31)
- 1985-10-02: WHEEL LOCK INFORMATION TWO TYPES OF LOCKS (86-3-102)
- 1985-10-02: NEW GASKETS: TRANSAXLE OIL PAN AND VALVE BODY COVER (86-7125-103)
- 1985-10-01: REMOVAL OF TIRE/WHEEL WEIGHT MARKER RESIDUE (85-140)
- 1985-10-01: AUTO TRANSMISSION COOLER LINE CHAFING ON HORN ASSEMBLY (85-142)
- 1985-10-01: GASKET MATERIAL INFORMATION (85-134)
- 1985-10-01: AUTO TRANSMISSION COOLER LINE CHAFING ON HORN ASSEMBLY (85-7-161)
- 1985-10-01: REMOVAL OF TIRE/WHEEL WEIGHT MARKER RESIDUE (86-3-101)
- 1985-09-30: TORQUE STEER TO THE RIGHT DIAGNOSIS ASSISTANCE (85-143)
- 1985-09-30: TORQUE STEER TO THE RIGHT DIAGNOSIS ASSISTANCE (86-3-100)
- 1985-09-25: PORT FUEL INJECTOR CLEANING ON VEHICLE PROCEDURE (85-132)
- 1985-09-25: PORT FUEL INJECTOR CLEANING ON VEHICLE PROCEDURE (85-6-245)
- 1985-09-13: COOLING FAN INOPERATIVE DAMAGED,BENT,DEFORMED TERMINAL (85-135)
- 1985-09-13: 3-2 DOWNSHIFT BUMP 440T4 TRANSAXLE,NEW P/N (85-139)
- 1985-09-13: COOLING FAN INOPERATIVE DAMAGED,BENT,DEFORMED TERMINAL (85-6-257)
- 1985-09-13: 3-2 DOWNSHIFT BUMP 440T4 TRANSAXLE,NEW P/N (85-7-157)
- 1985-08-19: TIRE ASSISTANCE WARRANTY & SERVICE ADJUSTMENTS (85-0-116)
- 1985-08-13: EXCHANGE PROCEDURE-ELECTRONIC INSTRUMENT CLUSTER (86-0-104)
- 1985-08-12: ELECTRONIC CONTROL MODULE EXCHANGE PROGRAM (85-6-221)
- 1985-08-06: 2ND GEAR START OUT NEW GOVERNOR ASSEMBLY (85-122)
- 1985-08-06: 2ND GEAR START OUT NEW GOVERNOR ASSEMBLY (85-7-151)
- 1985-08-02: CLARIFICATION AND REVISION OF DIAGNOSTIC ROUTINE,C/C SYSTEM (86-9)
- 1985-08-02: CLARIFICATION AND REVISION OF DIAGNOSTIC ROUTINE,C/C SYSTEM (85-9-117)
- 1985-07-26: TIRE AND WHEEL RUNOUT MEASURING AND REPAIRING (83-T-75)
- 1985-07-26: TIRE AND WHEEL RUNOUT MEASURING AND REPAIRING (85-3-133)
- 1985-07-25: CHOKE RELAY BUZZ REPLACE RELAY WITH NEW P/N (85-115)
- 1985-07-25: CHOKE RELAY BUZZ REPLACE RELAY WITH NEW P/N (85-6-243)
- 1985-07-11: BLOWN FUEL PUMP FUSE - OIL PRESS SWITCH WIRE CONTACT AXLE (85-6-231)
- 1985-06-28: DRIVE AXLE BOOT SEAL LEAK LOOSE CLAMP (85-106)
- 1985-06-28: DRIVE AXLE BOOT SEAL LEAK LOOSE CLAMP (85-4-104)
- 1985-06-27: ENGINE SERVICE PARTS IDENTIFIED 2.8L ENGINES (85-45)
- 1985-06-27: ENGINE SERVICE PARTS IDENTIFIED 2.8L ENGINES (85-6-217)
- 1985-06-24: ECM HARNESS: CHAFED OR CUT REPAIR PROCEDURE (85-104)
- 1985-06-17: PAINTING FLEX. PLASTIC PARTS VEHICLES W/PAINTED E/P OR TPO (85-2-138)
- 1985-06-13: INSTRUMENT CLUSTER (PRNDL) INDICATOR REPLACEMENT (85-8-136)
- 1985-06-12: TIMING GEAR NOISE/KNOCK 2.5L INFORMATION (83-T-18)
- 1985-06-12: TIMING GEAR NOISE/KNOCK 2.5L INFORMATION (85-6-208)
- 1985-06-05: SEALER HOT MELT PATCH SEALS BODY CRACKS OR JOINTS (85-2-140)
- 1985-05-20: TPS SPECIFICATIONS 1981-1985 SETTINGS (84-235)
- 1985-05-20: TPS SPECIFICATIONS 1981-1985 SETTINGS (85-6-214)
- 1985-05-16: CAMPAIGN: WIRING HARNESS MISROUTED (85-C-11)
- 1985-05-10: ELECTRONIC INSTRUMENT PANEL CLUSTER INFORMATION (85-8-127)
- 1985-05-03: UNIT REPAIR TRANS. THM 440T4 3-2 SHIFT CONTROL VALVE CHANGE (85-86)
- 1985-05-03: UNIT REPAIR TRANS. THM 440T4 3-2 SHIFT CONTROL VALVE CHANGE (85-7-139)
- 1985-04-29: NEW HYDRAULIC ENGINE MOUNTS CORRECT LOW SPEED RATTLE (85-88)
- 1985-04-29: GASKET MATERIAL FILLERS AND REINFORCEMENTS (85-0-112)
- 1985-04-29: SUBJECTIVE RATING SCALE PERFORMANCE/DISTURBANCE (85-0-113)
- 1985-04-29: NEW HYDRAULIC ENGINE MOUNTS CORRECT LOW SPEED RATTLE (85-6-199)
- 1985-04-22: VINYL TRIM AND VINYL TOP REPAIR & MAINTENANCE COMPOUNDS (85-10)
- 1985-04-22: PAINTED FLEXIBLE PLASTIC PARTS PAINT PROCEDURE (85-7)
- 1985-04-11: DIESEL-FUSE BLOCK/FUSE IDENTIFICATION 20AMP FUEL PUMP (85-82)
- 1985-04-11: DIESEL-FUSE BLOCK/FUSE IDENTIFICATION 20AMP FUEL PUMP (85-6-180)
- 1985-04-07: IDLE SPEED CONTROL DIAGNOSIS IDLE AIR CONTROL VALVE (85-72)
- 1985-04-07: IDLE SPEED CONTROL DIAGNOSIS IDLE AIR CONTROL VALVE (85-6-168)
- 1985-04-03: HIGH SHIFT EFFORT: 1-2 UPSHIFT 2-1 DOWNSHIFT 4 SPEED M/T (85-79)
- 1985-04-03: NO START / NO RUN BLOWN FUEL PUMP FUSE (85-80)
- 1985-04-03: NO START / NO RUN BLOWN FUEL PUMP FUSE (85-6-183)
- 1985-04-03: HIGH SHIFT EFFORT: 1-2 UPSHIFT 2-1 DOWNSHIFT 4 SPEED M/T (85-7-136)
- 1985-03-27: INOP INSTRUMENT PANEL LIGHTS GROUNDED RADIO LIGHT BULB (85-74)
- 1985-03-27: INOP INSTRUMENT PANEL LIGHTS GROUNDED RADIO LIGHT BULB (85-8-122)
- 1985-03-22: NEW FORWARD AND DIRECT CLUTCH THM 125C TRANSAXLE (85-64)
- 1985-03-22: NEW FORWARD AND DIRECT CLUTCH THM 125C TRANSAXLE (85-7-133)
- 1985-03-18: THM 125C TRANSAXLE CASE COVER OIL SLOT- MISDIAG. AS CRACK (85-67)
- 1985-03-18: SEAT BELT EXTENDER ACCESS AND AVAILABILITY (86-61)
- 1985-03-18: SEAT BELT EXTENDER INFORMATION (85-70)
- 1985-03-18: THM 125C TRANSAXLE CASE COVER OIL SLOT- MISDIAG. AS CRACK (85-7-128)
- 1985-03-18: SEAT BELT EXTENDER ACCESS AND AVAILABILITY (85-2-147)
- 1985-03-14: NON-REPAIRABLE POLICE- SPEEDOMETERS, REPLACEMENTS (85-44)
- 1985-03-14: NON-REPAIRABLE POLICE- SPEEDOMETERS, REPLACEMENTS (85-8-117)
- 1985-03-08: FRONT DISC BRAKE PADS LINING WEAR-NEW PADS P/N'S (85-77)
- 1985-03-08: FRONT DISC BRAKE PADS LINING WEAR-NEW PADS P/N'S (85-5-108)
- 1985-03-08: POWER STEERING PUMP O-RING CHANGE (85-41)
- 1985-03-08: POWER STEERING PUMP O-RING CHANGE (85-3-115)
- 1985-03-06: POWER STEERING LINE CONNECTION FITTING LEAK - SEAL DAMAGE (85-61)
- 1985-03-06: POWER STEERING LINE CONNECTION FITTING LEAK - SEAL DAMAGE (85-3-121)
- 1985-02-28: EXCESSIVE ALCOHOL IN FUEL POOR DRIVEABILITY (85-62)
- 1985-02-28: CANADIAN SERVICE MANUAL SUPPLEMENT REVISIONS (85-0-108)
- 1985-02-28: ENGINE SERVICE PARTS IDENTIFIED 2.8L ENGINES (85-6-151)
- 1985-02-28: INSTRUMENT CLUSTER EXCHANGE AND REPAIR PROGRAM (85-8-114)
- 1985-02-21: SPARK PLUG FOULING-FLOODING POOR DRIVEABILITY-INJECTORS (85-57)
- 1985-02-21: HOOD LATCH POP-UP SPRING INTERFERENCE (85-58)
- 1985-02-21: SPARK PLUG FOULING-FLOODING POOR DRIVEABILITY-INJECTORS (85-6-156)
- 1985-02-21: HOOD LATCH POP-UP SPRING INTERFERENCE (85-2-134)
- 1985-02-20: MIN. ACCEPTABLE OIL LEVELS TEST METHODS (85-54)
- 1985-02-20: MIN. ACCEPTABLE OIL LEVELS TEST METHODS (85-0-111)
- 1985-02-14: BRAKE SQUEAL TIGHTEN BRAKE PAD (85-52)
- 1985-02-14: BRAKE SQUEAL TIGHTEN BRAKE PAD (85-5-105)
- 1985-02-12: A/C SYSTEM REPLACEMENT O-RINGS CAPTURED-TYPE O-RINGS (85-114)
- 1985-02-12: A/C SYSTEM REPLACEMENT O-RINGS CAPTURED-TYPE O-RINGS (85-42)
- 1985-02-12: A/C SYSTEM REPLACEMENT O-RINGS CAPTURED-TYPE O-RINGS (85-1-115)
- 1985-02-01: PASSENGER CAR AND TRUCK IDENTIFICATION - 1985 MODELS (85-1)
- 1985-01-18: INJECTOR BALANCE TEST NEW PROD. MANUAL REVISION (85-0-109)
- 1985-01-15: 440-T4 TRANSMISSION-DEALER AUTHORIZED REPAIR (85-49)
- 1985-01-15: TECHINAL ASSISTANCE SYSTEM TOLL-FREE NUMBER AVAILABLE (85-0-104)
- 1985-01-15: 440-T4 TRANSMISSION-DEALER AUTHORIZED REPAIR (85-7-122)
- 1985-01-14: LOCKING WHEEL NUTS / PROPER WHEEL BALANCING (85-37)
- 1985-01-14: LOCKING WHEEL NUTS / PROPER WHEEL BALANCING (85-3-114)
- 1985-01-10: TORQUE CONVERTER CLUTCH SHUDDER THM 440-T4 TRANSAXLE (85-34)
- 1985-01-10: TORQUE CONVERTER CLUTCH SHUDDER THM 440-T4 TRANSAXLE (85-7-124)
- 1985-01-09: TRANSMISSION SIDE COVER BOLT & WASHER REPLACEMENT (85-36)
- 1985-01-09: TRANSMISSION SIDE COVER BOLT & WASHER REPLACEMENT (85-7-114)
- 1985-01-04: 2.5L ENGINE BLOCK REPLACEMENT OIL FILTER VALVE TRANSFER (83-I-99)
- 1985-01-04: OIL FILTER BYPASS VALVE 2.5L L4 ENGINE (85-30)
- 1985-01-04: OIL FILTER BYPASS VALVE 2.5L L4 ENGINE (85-6-143)
- 1985-01-04: 2.5L ENGINE BLOCK REPLACEMENT OIL FILTER VALVE TRANSFER (83-6-197)
- 1985-01-02: REMOVING WHEELS- CORROSION BUILD-UP CENTER HOLE HUB (85-28)
- 1985-01-02: CAMPAIGN:INTERFERENCE ENGINE MOUNT BRACKET TO OIL FILTER (85-C-04)
- 1985-01-02: CAMPAIGN:INTERFERENCE ENGINE MOUNT BRACKET TO OIL FILTER (5R07)
- 1985-01-02: REMOVING WHEELS- CORROSION BUILD-UP CENTER HOLE HUB (85-3-109)
- 1984-12-20: INTERMITTENT CHECK ENGINE CODE 22 OR 34 (85-23)
- 1984-12-20: INTERMITTENT CHECK ENGINE CODE 22 OR 34 (85-6-145)
- 1984-12-17: DIAGNOSIS USING ALDL FUEL FLOW ERRORS-INTEGRATOR/BLOCK LEARN (85-6-126)
- 1984-12-11: OIL AND FILTER CHARTS REVISED SPECS (85-0-107)
- 1984-12-06: AIR CONDITIONING NOISES V6 A/C BELT TENSION CHART (85-27)
- 1984-12-06: AIR CONDITIONING NOISES V6 A/C BELT TENSION CHART (84-1-116)
- 1984-11-21: BRAKE CALIPERS TO KNUCKLE CLEARANCE-REVISION (85-38)
- 1984-11-21: BRAKE CALIPERS TO KNUCKLE CLEARANCE-REVISION (85-5-101)
- 1984-11-12: LOWER BALL JOINT SERVICE TIPS FOR PROPER SERVICING (85-21)
- 1984-11-12: A/C HOSE AND CLAMP HOSE LEAK REPAIR (85-40)
- 1984-11-12: A/C HOSE AND CLAMP HOSE LEAK REPAIR (85-1-108)
- 1984-11-12: LOWER BALL JOINT SERVICE TIPS FOR PROPER SERVICING (85-3-107)
- 1984-11-10: ADDITION OF AUX ELECT. EQUIP. CONNECTIVE PARTS AVAILABLE (85-17)
- 1984-11-10: ADDITION OF AUX ELECT. EQUIP. CONNECTIVE PARTS AVAILABLE (85-8-109)
- 1984-11-09: V6 DIESEL FUEL FILTER SERVICE PARTS- NB9 FILTER SYSTEM (85-15)
- 1984-11-09: V6 DIESEL FUEL FILTER SERVICE PARTS- NB9 FILTER SYSTEM (85-6-124)
- 1984-11-08: HIGH LEVEL BRAKE LAMP INOPERATIVE (85-22)
- 1984-11-08: HIGH LEVEL BRAKE LAMP INOPERATIVE (85-8-112)
- 1984-10-24: CAMPAIGN:NO CLOSE THROTTLE LINK CLIP INTERFERENCE (85-C-01)
- 1984-10-17: FUEL LINE 'O' RING LEAKS FUEL ADDITIVE AFFECT (85-12)
- 1984-10-17: FUEL LINE 'O' RING LEAKS FUEL ADDITIVE AFFECT (85-6-117)
- 1984-10-15: SEAT BELT EXTENSIONS REVISED ODERING PROCEDURE (85-2-100)
- 1984-10-12: REMOTE MIRROR OFF COLOR PAINT REPAINT ESCUTCHEON (85-4)
- 1984-10-12: REMOTE MIRROR OFF COLOR PAINT REPAINT ESCUTCHEON (85-2-104)
- 1984-10-04: DIC/'CK.ENG.'LIGHTS STAY ON LAMP DRIVER CIRC.BD. LEFT IN (85-8-106)
- 1984-10-02: THM 125/125C TRANS.REVISIONS P/N CHANGES AND TRANS. IDENT. (85-9)
- 1984-10-02: THM 125/125C TRANS.REVISIONS P/N CHANGES AND TRANS. IDENT. (85-7-109)
- 1984-10-01: CAMPAIGN: NO CLOSE THROTTLE LINK CLIP INTERFERENCE (5A02)
- 1984-09-29: A/T OIL COOLER AND COOLER LINE FLUSHING (85-7-101)
- 1984-09-15: HIGH COLD HORN BLOWING EFFORT CUSTOM STEERING WHEELS (84-8-150)
- 1984-09-15: FRENCH LABEL INSTALLATION INSTRUCTIONS (PASS. CARS) (85-0-100)
- 1984-09-15: FRENCH LABEL INSTALLATION (PASS. & LIGHT DUTY TRUCKS) (85-0-101)
- 1984-08-13: EMERGENCY PARTS ORDERING PROCEDURE CLARIFICATION (86-48)
- 1984-08-02: POOR ENG.PERF.& DRIVEABILITY ADDITION OF NON OEM EQUIPMENT (85-2)
- 1984-08-02: POOR ENG.PERF.& DRIVEABILITY ADDITION OF NON OEM EQUIPMENT (85-6-100)
- 1984-07-26: GM GOODWRENCH 4.3 V6 DIESEL ENGINE COMPONENTS (84-164)
- 1984-07-26: GM GOODWRENCH 4.3 V6 DIESEL ENGINE COMPONENTS (84-6-209)
- 1984-07-16: DIESEL HOUSING PRESSURE COLD ADVANCE INFORMATION (84-187)
- 1984-07-16: DIESEL HOUSING PRESSURE COLD ADVANCE INFORMATION (84-6-197)
- 1984-06-29: TRANS. EXCHANGE PROGRAM FUNCTIONAL CHARACTERISTICS (84-168)
- 1984-06-27: TORQUE CONVERTER CLUTCH SHUDDER DIAGNOSIS,125C (84-171)
- 1984-06-27: REVISED:TORQUE CONVERT.CLUTCH DIAGNOSIS INFORMATION (82-T-125)
- 1984-06-27: REVISED:TORQUE CONVERT.CLUTCH DIAGNOSIS INFORMATION (83-T-41)
- 1984-06-27: REVISED: TORQUE CONVERT.CLUTCH DIAGNOSIS INFORMATION (83-T-53)
- 1984-06-27: TORQUE CONVERTER CLUTCH SHUDDER DIAGNOSIS,125C (84-7-147)
- 1984-05-22: CHECKING FOR CHAIN WEAR 125/125C/440T4 TRANS (84-146)
- 1984-05-22: CHECKING FOR CHAIN WEAR 125/125C/440T4 TRANS (84-7-136)
- 1984-04-26: CODE 44,45,55/CHECK ENGINE OXYGEN SENSOR TEST PROCEDURE (82-I-79)
- 1984-04-26: STARTING PROCEDURE WARM/COLD CHANGE IN OWNER'S MANUAL (84-6-194)
- 1984-04-26: CODE 44,45,55/CHECK ENGINE OXYGEN SENSOR TEST PROCEDURE (82-8-158)
- 1984-04-25: REDUCED PERFORMANCE ADD ON ELECTRICAL EQUIP. INFORMATION (84-167R)
- 1984-04-25: REDUCED PERFORMANCE ADD ON ELECTRICAL EQUIP. INFORMATION (84-6-223)
- 1984-04-04: BRAKE SYSTEM SERVICE INFORMATION (84-113)
- 1984-04-04: BRAKE SYSTEM SERVICE INFORMATION (84-5-105)
- 1984-02-16: 4.3L DIESEL ALUMINUM HEAD REMOVAL PROCEDURE (84-82)
- 1984-02-16: 4.3L DIESEL ALUMINUM HEAD REMOVAL PROCEDURE (84-6-146)
- 1984-02-15: A/C COMPRESSOR SHAFT SEAL INFORMATION (84-83)
- 1984-02-15: A/C COMPRESSOR SHAFT SEAL INFORMATION (84-1-117)
- 1984-01-15: REVISED: WIRE WHEEL NOISE INSTALL NYLON CLIPS (84-54)
- 1983-12-01: NON-REPAIRABLE POLICE SPEEDOMETERS, REPLACEMENTS (84-37)
- 1983-06-16: A/C COMPRESSOR INOPERATIVE INFORMATION (82-I-129)
- 1983-06-16: TORQUE CONVERTER CONTAMINATION TCC MODELS INFORMATION (82-I-95)
- 1983-06-16: TORQUE CONVERTER CONTAMINATION TCC MODELS INFORMATION (82-7-124)
- 1983-04-15: FLOOR PAN ASSEMBLY SERVICE REPLACEMENT PARTS (83-I-42)
- 1983-04-15: FLOOR PAN ASSEMBLY SERVICE REPLACEMENT PARTS (85-2-122)
- 1982-08-09: WINDSHIELD WASHER SPRAY- PATTERN ADJUSTMENT (82-2-128)
- 1982-08-06: MUST AND MILDEW ODOR CAUSE AND CORRECTION (82-I-102)
- 1982-08-06: MUST AND MILDEW ODOR CAUSE AND CORRECTION (82-0-116)
- 1981-12-14: ESCUTCHEON GASKET REPLACEMENT FRONT DOOR LOCK (85-24)
- 1981-12-14: ESCUTCHEON GASKET REPLACEMENT FRONT DOOR LOCK (85-2-124)