REVISED: REAR MAIN CRANK SERVICE SEAL INFORMATION. Chevrolet Celebrity 1983

For 1990-2009 cars

# REVISED: REAR MAIN CRANK SERVICE SEAL INFORMATION

#### Model and Year 1980-84 CAMARO, "S/T" TFUCKS, CITATION AND CELEBRITY

When service replacement of the rear main crankshaft seal in a 1980-84 2.8L V6 603 engine is required, a new rubber split seal should be used.

The new seal, unit P/N 14069889, has been released for all model service and replaces the current rope seal.

#### NOTICE: The installation instruction sheet (P/N 14069100)which is enclosed in the seal kit (P/N 14069889) may refer to the 'Cavalier' Shop Manual for removal and reinstallation of component parts. Disregard this and use the appropriate vehicle line shop manual.

The not under item 3 may read "loosening numbers 2, 3 and 4 main ....... This should be "loosening numbers 2 and 3 main .......

These items will be revised in future seal kits.

When installing the new rubber rear seal, the following procedure should be used:

1. Remove oil pan and oil pump.

2. Remove rear main bearing cap.

3. Remove upper and lower rope seal. Clean seal channel to remove any rope pieces and oil.

Loosening numbers 2 and 3 main bearings bolts may be necessary in both removing the upper rope seal and installing the new upper seal.

4. Apply a very thin coat of GM gasket sealing compound #1050026, or equivalent, to O.D. of rubber seal as shown in illustration. (Keep sealing compound off of seal lips.)

Roll seal into position in cylinder case; turning crank- shaft will help roll seal into position. A piece of shim stock must be used as a "shoe horn" between the seal O.D. and the edge of the block seal channel to prevent damaging the seal during installation.

Seal lip must be positioned inboard of the engine and the small dust lip to the flywheel side (see illustration below).

5. Apply GM gasket sealing compound in manner described above to other half of new seal and install in main bearing cap.

6. Apply a 1mm bead (approximately 1/32") of anerobic sealant #1052357, or equivalent, to the cap between the rear main seal end and the oil pan rear seal groove.

Keep sealant off the rear main seal, bearing and out of the drain slot.

7. Just prior to assembly, apply a light coat of engine oil on the crankshaft surface that will contact the seal.

8. Install rear main bearing cap. Torque bolts to 95 N.m (70 ft. lbs.). If other main bearings bolts were loosened, retorque as necessary.

9. Install oil pump and oil pan.

10. When running engine to confirm leak repair, insure the PCV system, including fresh air pipe from air cleaner to rocker cover is fully assembled.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.