SERVICE MANUAL UPDATE SECTION 4D DRIVE-AXLE. Chevrolet Celebrity 1989

For 1990-2009 cars

# SERVICE MANUAL UPDATE SECTION 4D DRIVE-AXLE

SERVICE MANUAL UPDATE

THE FOLLOWING FRONT DRIVE AXLE REPLACEMENT PROCEDURE REPLACES THE PROCEDURES FOUND IN THE 1988-89 A-CAR SERVICE MANUAL IN SECTION 4D, PAGES 1-4.

#### TOOLS REQUIRED:

J 34826 HUB NUT WRENCH (36MM) J 34754 INNER DRIVE JOINT SEAL PROTECTOR (MODIFIED) J 28733-A FRONT HUB SPINDLE REMOVER J 33008 AXLE SHAFT REMOVER J 29794 AXLE SHAFT REMOVAL EXTENSION J 2619-01 SLIDE HAMMER

REMOVE OR DISCONNECT

1. RAISE VEHICLE, REFER TO GENERAL INFORMATION (SECTION OA).

2. TIRE AND WHEEL ASSEMBLY, REFER TO TIRES AND WHEELS (SECTION 3E).

3. TIE ROD END COTTER KEY, NUT, AND JOINT FROM KNUCKLE, REFER TO FRONT SUSPENSION (SECTION 3C).

4. AXLE NUT AND WASHER USING J 34826 . DISCARD NUT

5. LOWER BALL JOINT PINCH BOLT, REFER TO FRONT SUSPENSION (SECTION 3C).

#### NOTICE: DRIVE AXLE SEAL PROTECTOR J 34754 SHOULD BE MODIFIED AND INSTALLED ON ANY DRIVE AXLE PRIOR TO SERVICE PROCEDURES ON OR NEAR THE DRIVE AXLE. FAILURE TO OBSERVE THIS CAN RESULT IN SEAL DAMAGE AND POSSIBLE JOINT FAILURE.

6. INSTALL J 34754

7. STABILIZER BOLTS AND STABILIZER

8. BRAKE LINE BRACKET BOLT

9. LOWER BALL JOINT, REFER TO FRONT SUSPENSION (SECTION 3C).

10. INSTALL J 28733-A AND REMOVE AXLE SHAFT FROM HUB.

11. J 28733-A FROM SPINDLE

12. AXLE SHAFT FROM TRANSAXLE USING J 3308, J 2619-01, AND J 29794.

13. J 34754

INSTALL OR CONNECT

1. AXLE TO TRANSAXLE

2. AXLE SHAFT IN HUB

3. LOWER CONTROL ARM BALL JOINT IN KNUCKLE, REFER TO FRONT SUSPENSION (SECTION 3C).

4. BRAKE LINE BRACKET

5. POSITION STABILIZER, INSTALL BOLTS, REFER TO FRONT SUSPENSION (SECTION 3C).

6. REINFORCEMENT BOLTS

7. LOWER BALL JOINT PINCH BOLT, REFER TO FRONT SUSPENSION (SECTION 3C).

8. DRIVE AXLE WASHER AND NEW NUT

TIGHTEN

. NUT TO 260 N.M (185 LB. FT.)

9. SEAT THE DRIVE AXLE INTO THE TRANSAXLE BY PLACING A SCREWDRIVER INTO THE GROOVE ON THE JOINT HOUSING AND TAPPING UNTIL SEATED.

10. VERIFY THAT DRIVE AXLE IS SEATED IN TRANSAXLE BY GRASPING ON THE HOUSING AND PULLING OUTBOARD, DO NOT GRASP AND PULL ON AXLE SHAFT.

11. TIE ROD END IN KNUCKLE, NUT, AND COTTER KEY, REFER TO FRONT SUSPENSION (SECTION 3C).

12. TIRE AND WHEEL ASSEMBLY, REFER TO TIRES AND WHEELS (SECTION 3E).

13. LOWER VEHICLE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.

COPYRIGHT 1989 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.<