DELCOTRON GROUND WIRE BROKEN NEW PLASTIC CLIP. Chevrolet Chevette 1983

For 1990-2009 cars

# DELCOTRON GROUND WIRE BROKEN NEW PLASTIC CLIP

Some Chevettes may exhibit Delcotron ground wire breakage due to vibration fatique caused by the Delcotron vibrating in its rubber mounts.

This condition can be corrected (see attached diagrams) by securing the ground wire in a plastic clip, P/N 8900116, and installing the clip in the specified hole on the back of Delcotron.

This change started in production on January 11, 1983 with V.I.N. DY156832.

Use applicable labor operation.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.