'CS' EMBLEM MISSING INSTALL ON DECK LID. Chevrolet Chevette 1984

For 1990-2009 cars

# 'CS' EMBLEM MISSING INSTALL ON DECK LID

#### VEHICLES AFFECTED: 1984 Chevette CS Series Vehicles

Some 1984 Chevette 'CS' Series may be missing the deck lid CS emblems. Chevette 'CS' Series vehicles can be identified by the appearance of the letter B at the fifth position of the vehicle serial number.

The CS emblem, P/N 14044267, can be ordered from WDDGM.

SERVICE PROCEDURE

1. Clean the area of the body surface where the emblem is to be applied, with a suitable solvent (oil-free naptha or alcohol). Use a clean cloth only.

2. Dry the surface with a clean cloth.

3. The body and emblem temperalure at the time of the emblem application should be 70 DEG to 90 DEG F. The adhesive surface must not be touched or brought in contact with any surface or foreign matter.

4. Apply the emblem to the LH side of the rear deck lid per the attached sketch and press firmly in place.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.