WRINKLES, BLISTERS AND BUBBLES IN FABRIC ROOF COVER. Chevrolet Chevette 1982

For 1990-2009 cars

# WRINKLES, BLISTERS AND BUBBLES IN FABRIC ROOF COVER

The correction of wrinkles, blisters or bubbles in the cover material can be accomplished by either a shrinking process or by partially removing the cover in the affected area and repositioning to draw the wrinkle out of the material. The latter method would be required to correct the more serious causes of wrinkles, while the shrinking method would be the practical approach for less severe wrinkles as well as blisters and bubbles.

Shrinking can be accomplished by two (2) methods:

METHOD 1

(1) Pierce each wrinkle, blister or bubble with a small hypodermic needle and withdraw any trapped air from inside the wrinkle, blister or bubble.

(2) Apply heat directly to the affected area with a heat gun.

#### NOTICE: Keep heat gun in motion when applying heat to roof cover material. Over-heating of vinyl will cause grain loss and permanent damage to the roof cover material.

When the material has warmed, it will begin to draw. At this point, the cover should be pressed against the roof panel. The heat will cause shrinking and reactivate the cement under the cover. The pressure on the top material will reestablish adhesion between the cover and the top.

METHOD 2

(1) This method resembles a clothes-pressing operation. Spread a wet shop towel over the affected area. Using a home-type laundry iron, pass the iron across the towel until towel becomes dry. If the iron used has heat control settings, the control should be set on "wool". Higher heat could permanently damage vinyl. The iron cannot be used without towel, since direct contact between the iron surface and the cover would result in distorting the cover grain pattern and create an objectionable gloss on the cover surface.

As in the previous method, the iron creates sufficient heat to draw the cover material and reactivate the cement. The pressure of the iron against the cover is sufficient to effect recementing of the cover to the top in the affected area.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.