DETONATION/ENGINE TIMING TIMING SPECIFICATIONS. Chevrolet Citation 1983

For 1990-2009 cars

# DETONATION/ENGINE TIMING TIMING SPECIFICATIONS

#### Model and Year: 1983 CELEBRITY

Some 1983 Celebritys with 2.8L V6 engines may exhibit engine detonation. On vehicles not repaired to the procedure outlined in the shop manual, retarding the base engine timing 4 DEG is permissible. Base engine timing is now 10 DEG BTDC, recommended base timing for cars with detonation is 60 BTDC. This change will alleviate the detonation problem.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.