CAMPAIGN:COMPACT SPARE WHEEL TO BRAKE CALIPER INTERFERENCE. Chevrolet Citation 1980

For 1990-2009 cars

# CAMPAIGN:COMPACT SPARE WHEEL TO BRAKE CALIPER INTERFERENCE

GENERAL MOTORS HAS DETERMINED THAT ON SOME 1980 CHEVROLET CITATION MODELS, THE COMPACT SPARE WHEEL, WHEN INSTALLED AT A FRONT WHEEL LOCATION, MAY BE IN CONTACT WITH THE BRAKE CALIPER WHICH MAY PREVENT THE VEHICLE FROM BEING DRIVEN. THIS INTERFERENCE CONDITION SHOULD BE OBVIOUS TO ANYONE INSTALLING THE WHEEL ON THE VEHICLE.

VEHICLES INVOLVED

ALL 1980 CHEVROLET CITATION MODELS ASSEMBLED AT WILLOW RUN AND TARRYTOWN WITHIN THE FOLLOWING PARAMETERS:

PLANT FROM THROUGH WILLOW RUN START OF PRODUCTION 1X085AW119277 TARRYTOWN START OF PRODUCTION 1X685AT108725 VEHICLES HAVE BEEN IDENTIFIED BY VEHICLE IDENTIFICATION NUMBER COMPUTER LISTINGS. THE LISTINGS HAVE BEEN FURNISHED TO INVOLVED DEALERS WITH THE CAMPAIGN BULLETIN. ANY DEALER NOT RECEIVING A COMPUTER LISTING WITH THE CAMPAIGN BULLETIN WAS NOT SHIPPED ANY INVOLVED VEHICLES.

OWNER NOTIFICATION

NO OWNER NOTIFICATION WILL BE REQUIRED SINCE ALL INVOLVED VEHICLES ARE IN DEALER STOCK.

DEALER CAMPAIGN RESPONSIBILITY

ALL INVOLVED VEHICLES ARE NOT TO BE SOLD BY THE DEALER UNTIL CAMPAIGN MODIFICATION HAS BEEN COMPLETED. SERVICE PROCEDURE

1. REMOVE COMPACT SPARE FROM VEHICLE STORAGE COMPARTMENT AND PLACE ON FLOOR WITH INBOARD SURFACE FACING UPWARDS (VALVE STEM TOWARDS FLOOR).

2. PLACE SPACER (PART NO. 9590681) ON THE INBOARD SURFACE OF THE WHEEL DISC WITH THE THREE PROTRUSIONS ON THE SPACER IN CONTACT WITH THE WHEEL AS ILLUSTRATED IN FIGURE 1.

3. UTILIZE THREE 9/16 INCH HEX HEAD BOLTS PLACED THROUGH THE SPACER AND INTO THE LUG HOLES OF THE WHEEL TO PROPERLY ORIENT THE SPACER AS SHOWN IN FIGURE 1.

#### NOTE: IF BOLTS LONGER THAN ONE INCH ARE UTILIZED, IT WILL BE NECESSARY TO EVELATE WHEEL AND TIRE ASSEMBLY SO THAT BOLTS ARE SUSPENDED BY WHEEL, INSURING PROPER SPACER ALIGNMENT.

4. USING ANY OF THE THREE SMALL HOLES IN THE SAPCER AS A GUIDE, DRILL AND DEBURR ONE HOLE THROUGH THE WHEEL USING A NO.11 (.191) DRILL.

#### NOTE: DRILLING AND RIVETING MUST BE DONE ONE HOLE AT A TIME TO INSURE PROPER ALIGNMENT AND A FLUSH RIVET HEAD.

5. PLACE SPECIAL STEEL RIVET (FURNISHED), THROUGH THE HOLE IN SPACER AND WHEEL. SECURE IN POSITION UTILIZING APPROPRIATE POP RIVET TOOL.

#### NOTE: A SCISSOR TYPE POP RIVET TOOL (FIGURE 2) IS RECOMMENDED TO INSURE PROPER RIVET INSTALLATION. IF A TOOL OF ANOTHER CONFIGURATION IS UTILIZED, IT IS ESSENTIAL THAT THE TOOL BE CAPABLE OF BEING POSITIONED PARALLEL TO THE SPACER WHEN SECURING THE RIVET.

6. REPEAT STEPS 4 AND 5 FOR THE REMAINING TWO SMALL HOLES IN THE SPACER.

7. REMOVE THE 9/16 INCH LOCATING BOLTS. INSPECT TO MAKE SURE ALL RIVETS ARE SECURELY INSTALLED AND THAT NONE OF THE RIVET HEADS EXTEND BEYOND THE SPACERS MOUNTING SURFACE.

8. INSTALL COMPACT SPARE IN VEHICLE STORAGE COMPARTMENT.

PARTS INFORMATION

PARTS REQUIRED TO COMPLETE THIS MODIFICATION ARE BEING SENT TO EACH CHEVROLET ZONE SERVICE DEPARTMENT ON A NO-CHARGE BASIS. PARTS WILL BE FURNISHED TO THE DEALER ON A NO-CHARGE BASIS.

QUANTITY PART NUMBER PER VEHICLE DESCRIPTION 9590681 1 PER VEHICLE WHEEL SPACER NPN 3 PER VEHICLE STEEL RIVETS

WARRANTY INFORMATION, FAILURE CODE, LABOR TIME ALLOWANCE, FAILED LABOR OPERATION AND CONDITION CODE

DEALERS ARE TO SUBMIT EACH CAMPAIGNED VEHICLE AS A SEPARATE CASE ON THE ONE-LINE WARRANTY CLAIM FORM, GSD-970.

THE CAMPAIGN FAILURE CODE, LABOR OPERATION NUMBER AND CONDITION CODE ARE TO BE SUBMITTED EXACTLY AS SHOWN ON THE EXAMPLE GSD-970 ONE-LINE CLAIM FORM INCLUDED IN THIS CAMPAIGN BULLETIN.

DEALERS SUBMITTING WARRANTY CLAIM APPLICATIONS ON THE CHEVROLET DEALER COMMUNICATION SYSTEM ARE TO SUBMIT CAMPAIGN CLAIMS VIA THE DEALER COMMUNICATIONS TERMINAL ACCORDING TO THE CAMPAIGN CLAIM PROCEDURE DOCUMENTED IN THE CHEVROLET "DEALER COMMUNICATION SYSTEM-OPERATION GUIDE." FAILURE CODE LABOR TIME FAILED LABOR CONDITION DESCRIPTION CODE ALLOWANCE OPERATION CODE 1A .3 HOURS 80C05 89 INSTALL SPACER USING SPECIAL STEEL POP RIVET FURNISHED

DEALERS WILL AUTOMATICALLY BE CREDITED 30% OF DEALER NET WHEN PARTS ARE FURNISHED, NO CHARGE BY CHEVROLET ($.30)

DEALERS WILL AUTOMATICALLY RECEIVE .1 HOURS DEALER ADMINISTRATIVE DETAIL ASSOCIATED WITH THIS CAMAPIGN.

ADMINISTRATIVE PROCEDURE

THE APPROPRIATE CAMPAIGN HANDLING AND ADMINISTRATIVE PROCEDURE MAY BE FOUND IN THE CHEVROLET SERVICE POLICIES AND PROCEDURE MANUAL, SECTION 5, PAGES 1 AND 2, DATED OCTOBER 1978 IN YOU DEALERSHIP.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.