INTERMEDIATE BAND APPLY PIN 125 TRANSMISSION. Chevrolet Citation 1983

For 1990-2009 cars

# INTERMEDIATE BAND APPLY PIN 125 TRANSMISSION

THE FOLLOWING IS A CALIBRATION CHECK AND ADJUSTMENT PROCEDURE FOR THE J-28535 INTERMEDIATE BAND APPLY PIN GAGE. FIG. 1. TO CHECK CALIBRATION: 1.HOLD J-28535 GAGE DOWN TIGHTLY AGAINST CHECKING BLOCK J-28535-50. ROTATE SHOULDER PIN TO ASSURE IT IS SEATED ON FLAT SURFACE. 2.WHITE LINE MUST BE ACROSS CENTER OF SIGHT HOLE. TO ADJUST CALIBRATION: 1.CALIBRATION PIN IS SECURED WITH LOCTITE. 2.TURN PIN WITH A SMALL PIPE WRENCH OR VISE-GRIP PLIERS. APPLYING HEAT TO LOCTITE WILL EASE TURNING EFFORT. 3.ADJUST PIN TO CENTER WHITE LINE IN SIGHT HOLE. 4.RESEAL PIN WITH LOCTITE NO. 290 OR EQUIVALENT. NOTICE: ONCE GAGE IS RECALIBRATED, DO NOT INTERMIX SHOULDER PINS WITH OTHER GAGE BODIES. STAMP OR MARK SHOULDER PIN AND GAGE BODY TO DENOTE THEY ARE MATCHED.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.