Intake Air Ducts. Chevrolet Corsica 1996

For 1990-2009 cars

### Removal Procedure

1. Loosen the clamps at the throttle body and the air cleaner assembly.
2. Remove the crankcase ventilation nipple from the ventilation port.
3. Remove the entire duct.

### Installation Procedure

1. Install the air cleaner outlet duct into the ventilation port and into the crankcase ventilation nipple.
2. Tighten the clamps at the throttle body and at the air cleaner assembly.