Torque Converter Assemble. Chevrolet Corsica 1996

For 1990-2009 cars

#### Tools Required

J 36850 Assembly Lubricant

1. Apply J 36850 (or equivalent) to a new oil seal ring (107) on the turbine shaft.
2. Apply J 36850 (or equivalent) to the turbine shaft splines (106).
3. Install the turbine shaft seal (107) onto the turbine shaft (106).

Caution: The torque converter weighs approximately 65 lbs. Personal injury may result if you lift the torque converter improperly.

4. Install the torque converter assembly (1).