Drive Sprocket Support Assemble. Chevrolet Corsica 1996

For 1990-2009 cars

#### Tools Required

• | J 8092 Driver Handle

• | J 28677 Sprocket Support-Needle Bearing Installer

1. Install the drive sprocket support assembly (109).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the four drive sprocket support bolts (114) into the case.

Tighten
Tighten the bolts to 24 N·m (18 lb ft).

3. If the bearing for the drive sprocket support is removed, perform the following steps:

3.1. | Assemble J 28677 and J 8092 .

3.2. | Use the assembled tools in order to install the drive sprocket support bearing assembly (108).