Case Cover and Gaskets Disassemble. Chevrolet Corsica 1996

For 1990-2009 cars

1. Use a flat blade screwdriver in order to disconnect the rod and clip assembly (701) from the manual valve (406).
2. Remove the case cover bolts and the two number 40 Torx™ head bolts.

Notice: Pry on the corner of the case side cover near the locating dowel pins (111), to prevent damage to the sealing surfaces.

3. Remove the case cover (401) from the case. A rubber mallet may be required in order to loosen the case cover from the case.
4. Set the case cover (401) aside on a clean work area with the case side of the cover facing upward.

Important: The 1-2 accumulator piston (421) and the pin (422) may have remained within the case cover (401).

5. Remove the 1-2 accumulator piston (421) and the pin (422).
6. Remove the 1-2 accumulator spring (419).

Notice: Do not damage the case flanges when removing the gaskets.

7. Remove the center gasket (415) from between the case and the case cover.
8. Remove the case cover gasket (416) from the case.