CAMPAIGN:SECONDARY HOOD LATCH INSTALL LATCH / SKID PLATE. Chevrolet Corsica 1987

For 1990-2009 cars

# CAMPAIGN:SECONDARY HOOD LATCH INSTALL LATCH / SKID PLATE

#### MODEL AND YEAR: 1987 CHEVROLET CORSICA AND BERETTA MODELS

This information supplements the Vehicles Involved, Owner Notification, Service Procedure and Claim Sections of Chevrolet Dealer Product Campaign 87CO2 dated December, 1986.

#### VEHICLES INVOLVED

# In addition to the vehicles involved as identified in the original campaign bulletin, the following units are also involved:

PLANT FROM THROUGH ----- ---- ------- Linden HE105504 HE106765 Wilmington HY101110 HY101930

Involved vehicles have been identified by Vehicle Identification Number Computer Listings. Any dealer not receiving a computer listing or parts with this campaign bulletin supplement has no additional involved vehicles currently assigned.

#OWNER NOTIFICATION

Owners of vehicles involved in this supplemental campaign will be notified of this campaign on their vehicles by Chevrolet Motor Division (see copy of Owner Letter included with this supplemental bulletin).

#PARTS INFORMATION

Parts required to complete this modification for vehicles involved in this supplemental bulletin are to be obtained from your local Branch office.

#Denotes change

# PART NUMBER DESCRIPTION USAGE QUANTITY/VEHICLE ----------- ----------- ----- ---------------- 10082277 Skid Plate Corsica & Beretta 1 (as required) 11508544 Screw Corsica & Beretta 2 (as required)

#### SERVICE PROCEDURE

#### CORSICA AND BERETTA

# 1. Raise hood and inspect catch surface of support for skid plate (P/N 10082277). If a skid plate is present and it is retained by either two (2) screws or two (2) rivets (see Figure 1) no further action is required. proceed to Step 10.

# If a skid plate is present and spot welded only (not retained by screws or rivets). locate and drill two (2) 9/64" pilot holes through skid plate and support as shown in Figure 1. Fasten skid plate securely using two (2) screws (P/N 11508544). Proceed to Step 7.

If no skid plate is present, proceed with the steps below.

2. Place skid plate (P/N 10082277) on catch surface of support. Nest skid plate fore-aft then slide plate to drivers side of vehicle until nested. It may be necessary to slide skid plate under plastic close out panel to assure proper nesting on the catch surface of support. (See Figure 1).

3. Using skid plate holes as a guide. center punch hole locations.

4. Drill two (2) 9/64" pilot holes.

5. Position plate and fasten securely using screw (P/N 11508544).

#### BERETTA ONLY

# 6. On vehicles produced before VIN HE105504 (Linden) or HY101110 (Wilmington), remove secondary latch assembly and replace with new latch assembly (P/N 10074017). Discard production locator screw (PIN 11508544) Figure 2. Vehicles built after above VIN's were produced with the revised latch assembly already in place.

CORSICA AND BERETTA

7. Check operation - While slowly lowering hood. secondary latch must slide down newly installed skid plate until fully engaged.

# Denotes change

CORSICA AND BERETTA

8. Should secondary latch rest on catch surface without sliding down sloped surface of skid plate, loosen screw (P/N 11503632) (2) places (See Figure 2). If not previously removed, remove and discard production locator screw (P/N 11508544) and adjust secondary latch forward slightly. Tighten screw (P/N 11503632) two (2) places. Check operation by slowly lowering hood as before.

9. If locator screw (P/N 11508544) is removed for either secondary latch replacement (Beretta) or for secondary latch adjustment (Corsica or Beretta), a new (P/N 11508544) locator screw must be installed. It may be necessary to first drill a 9/64" pilot hole if secondary latch assembly required adjustment for proper operation.

10. Install campaign identification label.

#### CLAIM INFORMATION

Submit a product campaign claim with the information included below.

* *** FAILED PARTS LABOR LAB OTH NET REPAIR PERFORMED PC PART NO. ALLOW FC OP HRS HRS AMT ---------------- -- ------- ----- -- -- --- --- --- INSPECTION ONLY 00 V3782 0.2 0.1 $0.00 CORSICA & BERETTA

INSTALL SCREWS ONLY 00 V3783 0.2 0.1 $0.59 CORSICA & BERETTA

INSTALL SKID PLATE 00 V3780 0.3 0.1 $2.54 CORSICA & BERETTA

INSTALL SKID PLATE 00 V3781 0.4 0.1 $7.41 SECONDARY HOOD LATCH BERETTA ONLY

*Campaign Administrative Allowance ***The anounts listed in the "Net Amount" column represent 30% of parts cost when parts are furnished no charge by Chevrolet.

Dealers will automatically receive the correct labor and material allowance based on the labor operation performed.

Refer to the Chevrolet Claims Processing manual for details on Product Campaign Claim submission.

# Denote Change

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.