Fastener Tightening Specifications. Chevrolet Corsica 1996

For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Coolant Pump Pulley to Pump Bolts 2.2L (4 cyl.) | 30 | 22 | --
Coolant Pump Pulley to Pump Bolts 3.1L (6 cyl.) | 25 | 18 | --
Coolant Pump to Block Bolts 2.2L (4 cyl.) | 25 | 18 | --
Coolant Pump to Front Cover Bolts 3.1L (6 cyl.) | 10 | -- | 89
Fan Assembly Motor to Fan | 3.3 | -- | 29
Fan to Radiator Support Bolt | 11 | -- | 97
Radiator to Radiator Support Bolts | 10 | -- | 89
Surge Tank Screw | 9 | -- | 80
Surge Tank Cap | 4 | -- | 35
Surge Tank Inlet Pipe to Block Fitting 3.1L (6 cyl.) | 21 | 15 | --
Temperature Sending or Gauge Unit | 27 | 20 | --
Thermostat Housing 2.2L (4 cyl.) | 10 | -- | 89
Thermostat Housing 3.1L (6 cyl.) | 25 | 18 | --
Transaxle Oil Cooler Pipe Connections | 30 | 22 | --