FRONT STABILIZER BAR LINK SQUEAK NOISE/REPLACE LINK ASSY. Chevrolet Corsica 1990

For 1990-2009 cars

# FRONT STABILIZER BAR LINK SQUEAK NOISE/REPLACE LINK ASSY

#### VEHICLES AFFECTED: 1990 L-CAR GTZ (RPO Z04)

#### CONDITION:

Some 1990 L-car GTZ models (RPO Z04) assembled prior to VIN LY157125 may exhibit a squeak/squawk noise condition that is most evident when turning the steering wheel 30 degrees right or left of centre with the vehicle stationary.

#### CAUSE:

May be the result of inadequate lubrication in the stabilizer bar links.

#### CORRECTION:

Replace both stabilizer bar links with new links, P/N 17999125 following applicable Shop Manual procedure.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.