SERVICE BRAKE PART NUMBER (REDUCES PEDAL EFFORT). Chevrolet Corsica 1988

For 1990-2009 cars

# SERVICE BRAKE PART NUMBER (REDUCES PEDAL EFFORT)

#### Model and Year: 1987-88 BERETTA, CORSICA

Some owners of 1987 and 1988 Beretta, Corsica vehicles may express dissatisfaction with brake pedal effort, Lower pedal effort can be accomplished by replacing the original front brake pads with a new lining material. Customers should be advised that some brake squeal may be associated with the new lining material, particularly in warm weather and periods of heavy brake usage. The new linings are to be used for pedal effort complaint vehicles only and not as a general replacement part. DO NOT refinish the rotors when installing the new pads unless absolutely necessary due to external damage. Light surface rust and circumferential grooves in the rotor faces up to a depth of 0.015 inch, caused by the original pads, will not adversely affect brake performance.

#### NEW ORIGINAL

LININGS 18015497 12321424

Use applicable labor time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.