SMU - SECTION 6E3 - C2 - FUEL METERING SYSTEM - REVISED. Chevrolet Corsica 1995

For 1990-2009 cars

# SMU - SECTION 6E3 - C2 - FUEL METERING SYSTEM - REVISED

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6E3-C2 - FUEL METERING SYSTEM-REVISED FUEL PRESSURE RELIEF PROCEDURE

#### MODELS: 1995 CHEVROLET BERETTA, CORSICA WITH 2.2L ENGINE (VIN 4 - RPO LN2)

THIS BULLETIN IS BEING ISSUED TO REVISE THE FUEL PRESSURE RELIEF PROCEDURE IN THE 1995 CHEVROLET BERETTA/CORSICA SERVICE MANUAL. REPLACE THE FUEL PRESSURE RELIEF PROCEDURE LISTED ON PAGE 6E3-C2-8 WITH THE FOLLOWING PROCEDURE:

FUEL PRESSURE RELIEF PROCEDURE

1. LOOSEN FUEL FILLER CAP TO RELIEVE TANK PRESSURE (DO NOT TIGHTEN AT THIS TIME). 2. RAISE VEHICLE. 3. DISCONNECT FUEL PUMP ELECTRICAL CONNECTOR. 4. LOWER VEHICLE. 5. START ENGINE AND RUN UNTIL FUEL SUPPLY REMAINING IN FUEL PIPES IS CONSUMED. ENGAGE STARTER FOR 3.0 SECONDS TO ASSURE RELIEF OF ANY REMAINING PRESSURE. 6. RAISE VEHICLE. 7. CONNECT FUEL PUMP ELECTRICAL CONNECTOR. 8. LOWER VEHICLE. 9. DISCONNECT NEGATIVE BATTERY CABLE TO AVOID POSSIBLE FUEL DISCHARGE IF AN ACCIDENTAL ATTEMPT IS MADE TO START THE ENGINE.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.