Crankshaft Rear Oil Seal and Housing Removal. Chevrolet Corsica 1996

For 1990-2009 cars

1. Remove the flywheel. Refer to Flywheel Removal.

Notice: Do not damage the crankshaft surface when prying out the crankshaft rear oil seal.

2. Remove the crankshaft rear oil seal. Pry the crankshaft rear oil seal out with a suitable pry tool.
3. Clean the crankshaft rear oil seal to engine block mating surface.
4. Inspect the following areas:

• | Inspect the seal bore for nicks

• | Inspect the seal bore for burrs

• | Inspect the seal mating surface on the crankshaft for nicks