Water Pump Installation. Chevrolet Corsica 1996

For 1990-2009 cars

1. Install the coolant pump gasket to the engine.
2. Install the coolant pump to the engine.
3. Apply sealant to the bolt threads, use GM P/N 1052080 (or equivalent).
4. Install the coolant pump attaching bolts.

Tighten
Tighten the coolant pump attaching bolts to 25N·m (18 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.