Shifts 3-1 at High Speeds for Passing Gear. Chevrolet Corsica 1996

For 1990-2009 cars

Checks | Cause
--- | ---

Governor (4) or Speed Sensor (4) (depending on model)

• | The cover is worn (9)

• | The thrust washer is missing (6)

• | The governor seal is worn or cut (7)

• | The governor spring is not seated (4)

• | The governor weights are binding on the pin (4)

• | A ball is missing (4)

• | The governor driven gear is stripped (4)

Intermediate Servo (128-137) | The intermediate servo is sticking (129-134)
Direct Clutch Orifice Controlled by #2 Checkball | Restricted orifice

1-2 Accumulator (419-422)

• | The piston is missing (421)

• | A seal is leaking (420)