Park Lock Pawl Actuator Replacement. Chevrolet Corsica 1996

For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to General Vehicle Lifting and Jacking in General Information.
2. Remove the oil pan and the oil pan gasket.
3. Remove the oil pan filter and the seal.
4. Remove the transmission fluid level indicator stop bracket.
5. Remove the spring shaft retainer.
6. Remove the parking pawl actuator bracket.
7. Remove the clip.
8. Remove the manual shift shaft pin.
9. Remove the manual valve with the retainer rod.
10. Remove the manual valve pin.
11. Remove the parking pawl spring.

### Installation Procedure

1. Install the parking pawl spring.
2. Install the manual valve pin.
3. Install the manual valve with the retainer rod.
4. Install the manual shift shaft pin.
5. Install the clip.
6. Install the parking pawl actuator bracket.
7. Install the spring shaft retainer.
8. Install the transmission fluid level indicator stop bracket.
9. Install the oil pan filter and the seal.
10. Install the oil pan and the gasket.
11. Lower the vehicle.
12. Adjust the oil level.
13. Inspect the shift linkage.