Cooler Fitting Connectors Assemble. Chevrolet Corsica 1996

For 1990-2009 cars

1. Apply thread sealer 12345382 to the threads of the cooler fitting (17).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Hand start and install the cooler fitting before you tighten the fitting to the case cover.

Tighten
Tighten the cooler fitting to 38 N·m (23 lb ft).