DTC P0602 Control Module Not Programmed. Chevrolet Corsica 1996

For 1990-2009 cars

### Circuit Description

The PCM used in this vehicle utilizes an Electrically Erasable Programmable Read-Only Memory (EEPROM). The EEPROM contains program information and the calibrations required for engine, Transaxle, and Powertrain diagnostics operation.

Unlike the PROM used in past applications, the EEPROM is not replaceable. When the PCM is replaced or a calibration update is required, the PCM must be programmed using Techline equipment (Tech 1 or Tech 2 scan tool). Refer to On-Vehicle Service in Powertrain Control Module and Sensors for the EEPROM programming procedure.

### Conditions for Setting the DTC

• | The PCM does not contain the correct program required to operate the vehicle.

### Action Taken When the DTC Sets

• | The PCM will not illuminate the malfunction indicator lamp (MIL).

• | The PCM will store conditions which were present when the DTC set as Failure Records data only. This information will not be stored as Freeze Frame data.

### Conditions for Clearing the MIL/DTC

• | A History DTC will clear after 40 consecutive warm-up cycles have occurred without a malfunction.

• | The DTC can be cleared by using the scan tool Clear Info function.

#### DTC P0602 - PCM Not Programmed

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic System Check performed? | -- | Go to Step 2 | Go to Powertrain OBD System Check

2

1. Program the PCM with correct software. Refer to On-Vehicle Service in Powertrain Control Module and Sensors for procedures.
2. Retest for DTC P0602.

Did DTC P0602 set?

--

Go to Step 3

Repair complete

3 | Replace the PCM. Important: The replacement PCM must be programmed. Refer to Replacement/Programming. Is action complete? | -- | Go to Powertrain OBD System Check | --