FRONT SEAT BELT STAINED BY ACOUSTIC PATCH MATERIAL. Chevrolet Corsica 1988

For 1990-2009 cars

# FRONT SEAT BELT STAINED BY ACOUSTIC PATCH MATERIAL

#### SUBJECT: FRONT SEAT BELTS STAINED BY ACOUSTIC PATCH MATERIAL (STAINED SEAT BELTS) REMOVE ACOUSTIC PATCH AND CLEAN AREA

#### VEHICLES AFFECTED: 1987-88 L-CAR

Some 1987-88 "L" Models front seat belts may be stained by acoustic patch sealer. The patch is located above the seat belt retractors.

If owner comments on stained front seat belts are received, the following procedure should be used for both driver and passanger front seat belts, even if only one side has this condition.

1. Remove trim as required to gain access to seat belt retractors.(See Shop Manual)

2. Remove acoustic patch from retractor area and clean area completly of all acoustic patch material on both left and right sides. DO NOT replace acoustic patch.

3. Install new seat belt assembly per instructions in Shop Manual if webbing is stained.

Use the most applicable labour operation from the Canadian Labour Time Guide and claim as follows:

Right Side .6 Hr. plus .1 Hr. per side cleaning Left Side .6 Hr. plus .1 Hr. per side cleaning

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.