Torque Converter Fluid Seal Removal. Chevrolet Corsica 1996

For 1990-2009 cars

#### Tools Required

• | J 23129 Axle Seal Remover

• | J 6125-1B Slide Hammer

1. Assemble J 6125-1B and J 23129 .

Important: Do not damage the transmission case during removal of the seal assembly for the torque converter from the case.

2. Use the assembled tools in order to remove the oil seal assembly (115) for the torque converter from the case:

• | As an alternate removal method, use a large, flat blade screwdriver in order to pry out the oil seal assembly for the torque converter from the case.

• | Use a block of wood to pry against.