Camshaft and Bearings Cleaning and Inspection. Chevrolet Corsica 1996

For 1990-2009 cars

#### Tools Required

J 8001 Dial Indicator Set

1. Measure the camshaft journals with a micrometer.

If journals are more than 0.025 mm (0.0010 in) out-of-round, replace the camshaft.

2. Measure camshaft runout using J 8001 .

2.1. | Mount the camshaft in V-blocks between centers.

2.2. | Use the J 8001 in order to check the intermediate camshaft journal

3. If runout exceeds 0.065 mm (0.0026 in), camshaft is excessively bent and should be replaced.