LOOSE LOCK PILLER MOLDING REPAIR PROCEDURE-BERETTA ONLY. Chevrolet Corsica 1988

For 1990-2009 cars

# LOOSE LOCK PILLER MOLDING REPAIR PROCEDURE-BERETTA ONLY

#### VEHICLES AFFECTED: 1988-89 BERETTAS

Loose lock pillar finishing moulding may be reattached to the lock pillar by adding tape to the two lower attaching tabs. Tape must cover both sides of the tabs. (See Illustration).

Thickness of the tape will determine the amount of retention, therefore, a minimum of 1/8" thickness is required for each side of both lower tabs.

Use 3M 06375 foam tape, or cloth back body tape or equivalent.

Use most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.