Engine Coolant Temperature Sensor Replacement. Chevrolet Corsica 1996

For 1990-2009 cars

### Removal Procedure

Notice: Use care when handling the coolant sensor. Damage to the coolant sensor will affect the operation of the fuel control system.

1. Turn the ignition switch OFF.
2. Relieve the coolant system pressure.
3. Disconnect the ECT sensor electrical connector (1).
4. Carefully back out the ECT sensor (2).

### Installation Procedure

1. Coat the threads (only) with sealer.
2. Install the ECT sensor (2).

Tighten
Tighten the ECT sensor to 25 N·m (18.5 lb. ft.).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Connect the ECT sensor electrical connector (1).
4. Refill the engine coolant system.