REAR SIDE MARKER LAMP WATER MOISTURE ENTRY (BERETTA ONLY). Chevrolet Corsica 1988

For 1990-2009 cars

# REAR SIDE MARKER LAMP WATER MOISTURE ENTRY (BERETTA ONLY)

#### Model and Year: 1987-88 L CAR (BERETTA ONLY)

#### TO: ALL CHEVROLET DEALERS:

Side marker lamps or sockets may corrode as a result of water/moisture entry. A new rear side marker lamp wiring harness entered production effective with VIN Y616022 at Wilmington and VIN E636202 at Linden assembly plants. This new harness has mastic grease in the lamp sockets and can be used on earlier models.

The part number of the new harness is 12081598.

Labor Operation Number: N6560 Labor Time: . 5 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.