Park System Components Disassemble. Chevrolet Corsica 1996

For 1990-2009 cars

1. Use a drift pin and a mallet in order to remove the pin (702) connecting the detent lever to the shaft.

Notice: Use a piece of wood or other protective material when you remove the manual shaft pin, to prevent damage to the case.

2. Use a long flat blade screwdriver in order to remove the pin (713) connecting the manual shaft to the case.
3. Hold the detent lever (703) and pull the manual shaft park lock actuator rod (704) out of the driven sprocket support (602) and the case (15).
4. Remove the manual detent lever (703) and the manual valve rod (701).