Oil Pan Installation. Chevrolet Corsica 1996

For 1990-2009 cars

1. Apply a 5 mm (0.193 in) diameter bead of GM P/N 12346286 or equivalent to the oil pan side sealing flanges.
2. Apply GM P/N 12346286 or equivalent to the oil pan surface that contacts the engine front cover.
3. Install a new oil pan rear seal. Apply a small amount of GM P/N 12346286 or equivalent to the oil pan rear seal ears.
4. Install the oil pan.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the oil pan nuts.

Tighten
Tighten the oil pan nuts to 10 N·m (89 lb in).

6. Install the oil pan bolts.

Tighten
Tighten the oil pan bolts to 10 N·m (89 lb in).