Catalytic Converter Replacement. Chevrolet Corsica 1996

For 1990-2009 cars

## Catalytic Converter Replacement w/o Manifold Pipe

### Removal Procedure

1. Raise the vehicle.
2. Support the three way catalytic converter.
3. Support the exhaust manifold pipe assembly.
4. Remove the three way catalytic converter from the intermediate pipe.
5. Remove the three way catalytic converter from the exhaust manifold pipe assembly.
6. Remove the three way catalytic converter and seals.
7. Clean the flange surfaces.

### Installation Procedure

1. Install the three way catalytic converter seals.
2. Install the three way catalytic converter to the intermediate pipe assembly.
3. Install the three way catalytic converter to the exhaust manifold pipe assembly.
4. Lower the vehicle.

## Catalytic Converter Replacement w/ Manifold Pipe

### Removal Procedure

1. Raise the vehicle.
2. Support the three way catalytic converter.
3. Remove the intermediate pipe from the three way catalytic converter.
4. Remove the exhaust manifold pipe assembly from the exhaust manifold.
5. Remove the exhaust manifold seal and the three way catalytic converter seal.
6. Clean the flange surfaces.

### Installation Procedure

1. Install the exhaust manifold seal and the three way catalytic converter seal.
2. Install the exhaust manifold pipe assembly to the exhaust manifold.
3. Install the intermediate pipe to the three way catalytic converter.
4. Lower the vehicle.