REAR GLASS REVEAL MOLDING LOOSE/NOT FLUSH FIT. Chevrolet Corsica 1988

For 1990-2009 cars

# REAR GLASS REVEAL MOLDING LOOSE/NOT FLUSH FIT

BACKGLASS REVEAL MOULDING LOOSE/NOT FLUSH

#### VEHICLES AFFECTED: 1987-88 "L" CAR -----------------

Comments have been made that the backglass reveal mouldings are loose or not flush on the subject vehicles.

Service correction for this condition consists of installing a revised lace. The part numbers for the revised laces are 10092382 for the coupe and 10092380 for the sedan.

#### SERVICE PROCEDURE

1. Remove backglass.

2. Clean edge of glass.

3. Press the new lace onto the glass. (Butyl is present at the base of the slot of the lace).

4. Apply urethane to glass.

5. Reinstall glass and lace assembly into the opening.

Labour Operation Number: B8520

Labour Time : 1.3 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.