MANUAL 4-WAY SEAT ADJUSTER HANDLE INOPERATIVE. Chevrolet Corsica 1988

For 1990-2009 cars

# MANUAL 4-WAY SEAT ADJUSTER HANDLE INOPERATIVE

#### VEHICLES AFFECTED: 1988 CORSICA, TEMPEST AND BERETTA MODELS BUILT PRIOR TO20 FEB. 1987

Owners of some early production 1988 Corsica, Tempest and Beretta models built before 20 February, 1987 may comment on the 4-way seat adjuster handle becoming disengaged from the seat adjuster assembly.

Should this condition occur DO NOT repair the adjuster assembly REPLACE THE COMPLETE seat adjuster assembly with a new one.

Use the most applicable labour operation from the Canadian Labour Time Guide and claim 0.3 hours per side.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.