Governor Replacement. Chevrolet Corsica 1996

For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to General Vehicle Lifting and jacking in General Information.
2. Remove the vehicle speed sensor (VSS) assembly. Refer to Vehicle Speed Sensor Replacement .
3. Remove the governor.
4. Remove the governor compression ring.
5. Remove the governor shaft seal.
6. Remove the governor shaft bushing and the screen.

### Installation Procedure

1. Install the governor shaft bushing and the screen.
2. Install the governor shaft seal.
3. Install the governor compression ring.
4. Install the governor.
5. Install the vehicle speed sensor (VSS) assembly. Refer to Vehicle Speed Sensor Replacement .
6. Lower the vehicle.
7. Adjust the oil level.