Transmission Support Replacement. Chevrolet Corsica 1996

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 28467-360 Engine Support Fixture

1. Disconnect the negative battery cable. Refer to

   Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

   in General Information.
2. Remove the air intake duct. Refer to Air Cleaner (2.2L) in Engine Controls.
3. Remove the TV cable, if equipped. Refer to Automatic Transmission Throttle Valve Cable Replacement .
4. Remove the power brake booster line.
5. Remove the hose.
6. Install the J 28467-360 to the transmission. Raise the engine just enough to unload the transmission mounts.
7. Raise the vehicle. Support the vehicle. Refer to General Vehicle Lifting and Jacking in General Information.
8. Remove the engine mount strut.
9. Remove the left front tire and the wheel assembly. Refer to Wheel Removal in Tires and Wheels.
10. Remove the left splash shield.
11. Remove the crossmember.
12. Remove the left front ABS wheel speed sensor connector.
13. Remove the harness from the suspension support.
14. Remove the left front ball joint. Refer to Ball Joint in Front Suspension.
15. Remove the left stabilizer bushing nuts. Refer to Stabilizer Shaft in Front Suspension.
16. Remove the stabilizer shaft from the left lower control arm. Refer to Stabilizer Shaft in Front Suspension.
17. Remove the left suspension support. Refer to Front Suspension.
18. Remove the left side drive axle from the transmission. Refer to Drive Axle in Drive Axle On-Vehicle Service.
19. Remove the transmission cooler pipes. Plug in order to prevent leakage. Refer to Automatic Transmission Oil Cooler Pipes Replacement .
20. Remove the P/S lines from the P/S gear. Plug in order to prevent leakage.
21. Remove the transmission mount to body bolts.
22. Remove the pipe expansion bolt from the transmission support assembly.
23. Lower the engine and the transmission assembly just enough to be able to remove the transmission support assembly and the mount assembly.
24. Remove the transmission mount from the transmission support assembly.
25. Remove the transmission support assembly bolts.
26. Remove the transmission support assembly.

### Installation Procedure

1. Position the transmission support assembly into the vehicle.
2. Install the transmission support assembly bolts.

Tighten
Tighten the bolts to 75 N·m (55 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the transmission mount to the transmission support assembly.
4. Raise the engine and the transmission assembly.
5. Install the transmission mount to body bolts.

Tighten
Tighten the bolts to 66 N·m (49 lb ft).

6. Install the transmission pipe expansion bolt to the transmission support assembly.

Tighten
Tighten the bolt to 55 N·m (41 lb ft).

7. Install the P/S lines to the P/S gear.
8. Install the transmission cooler lines. Refer to Automatic Transmission Oil Cooler Pipes Replacement .
9. Install the left drive axle to the transmission. Refer to Drive Axle in Drive Axle On-Vehicle Service.
10. Install the left suspension support. Refer to Front Suspension.
11. Install the stabilizer shaft to the left lower control arm. Refer to Stabilizer Shaft in Front Suspension.
12. Install the left stabilizer bushing nuts. Refer to Stabilizer Shaft in Front Suspension.
13. Install the left front ball joint. Refer to Ball Joint in Front Suspension.
14. Route and connect the left front ABS wheel speed sensor.
15. Install the crossmember.
16. Install the left splash shield.
17. Install the left front tire and the wheel assembly. Refer to Wheel Installation in Tires and Wheels.
18. Install the engine mount strut.
19. Lower the vehicle.
20. Remove the engine support fixture.
21. Install the power brake booster line.
22. Install the hose.
23. Install the TV cable, if equipped. Refer to Automatic Transmission Throttle Valve Cable Replacement .
24. Install the air intake duct. Refer to Air Cleaner (2.2L) in Engine Controls.
25. Connect the negative battery cable.
26. Adjust the P/S oil level. Refer to Checking and Adding Fluid in Power Steering Gear and Pump.
27. Adjust the TV cable. Refer to Automatic Transmission Throttle Valve Cable Adjustment .
28. Check the oil level.
29. Inspect the suspension alignment. Refer to J Car Alignment Specifications in Wheel Alignment.
30. Inspect the transmission for oil leaks.