Case Components Assemble. Chevrolet Corsica 1996

For 1990-2009 cars

1. Apply GM P/N 12345382 on cup plug (118).
2. Using a drift and a mallet, install a new cup plug for the park pawl shaft into the case.
3. Apply GM P/N 12345382 to governor pressure pick-up plug (119).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the governor pressure pick-up plug (119) in the case.

Tighten
Tighten the plug to 11 N·m (8 lb ft).