LOW OIL PRESSURE READINGS (NEW SENDER MAY REPAIR P/N). Chevrolet Corsica 1987

For 1990-2009 cars

# LOW OIL PRESSURE READINGS (NEW SENDER MAY REPAIR P/N)

LOW OIL PRESSURE READINGS

#### VEHICLES AFFECTED: 1987-88 L-CARS W/2.8L AND 2.0L WITH GAGE ------------------ CLUSTER (U21/UB3)

The oil pressure gage on some 1987-88 L-cars may read in the red warning zone during a hot idle condition. This could be a false indication of an oil pressure condition due to an improper sender calibration.

Engine oil pressure should be checked using a verified accurate external gauge installed in place of the oil pressure sender. The minimum oil pressure measured at hot idle should be 41 kpa (6 PSI) and this pressure should immediately increase when engine RPM is increased. If these readings are bad, there may be a problem within the engine oil distribution system.

If the engine has proper oil pressure, a new oil pressure sender can be installed which redefines the gauge reading at the low end of the scale. This should give the customer a more accurate warning of low engine oil pressure.

#### 1987 and 1988 (Below VIN 500000)

10068576 - 2. 8L (LB6) Vin Code (W) Engine

#### 1988 (Above VIN 500000)

1647135 - 2.0L (LL8) Vin Code (1) Engine 1647136 - 2.8L (LB6) Vin Code (W) Engine

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.