1-2 Accumulator Assemble. Chevrolet Corsica 1996

For 1990-2009 cars

1. Remove the 1-2 accumulator piston seal (420) from the 1-2 accumulator piston (421).

Important: Lubricate the new seal with TRANSJEL™ or equivalent in order to ease further installation.

2. Install a new 1-2 accumulator piston seal (420) onto the 1-2 accumulator piston (421).
3. Slide the 1-2 accumulator piston pin (422) into the case cover (401) with the chamfered end away from the case cover (401).
4. Slide the 1-2 accumulator piston (421) into the case cover (401) with the chamfered end away from the case cover (401).
5. Use TRANSJEL™ or equivalent in order to hold the 1-2 accumulator piston (421) to the case cover.