CATALYTIC CONVERTER EXHAUST ODOR-NEW P/N AVAILABLE. Chevrolet Corsica 1987

For 1990-2009 cars

# CATALYTIC CONVERTER EXHAUST ODOR-NEW P/N AVAILABLE

SPECIFIC A, J AND L CARLINES MAY EXHIBIT A HIGHER THAN NORMAL CATALYTIC CONVERTER ODOR DURING VEHICLE OPERATION. THIS ODOR CONDITION CAN BE REDUCED BY INSTALLING A SERVICE CATALYTIC CONVERTER AS SPECIFIED BELOW: VIN BREAKPOINTS ARE FOR 1987 "J" AND 1988 "L" CARS. CARLINE ENGINE (VIN CODE) CONVERTER VIN BREAK PT. _________ __________________ __________ ________________ A V-6, 2.8L (W) 25104019 DIVISIONS. VIN BREAKPOINTS CHEV 88 MODEL YEAR. START-UP BUICK OLDS PONT CANADA J L-4, 2.OL (1) 25103456 DIVISIONS VIN BREAKPOINTS CHEV H7183332 CHEV HJ201273 CHEV HK140800 OLDS HK320062 BUICK HK440902 J (Z24 MODEL) V-6, 2.8L (W) 25104027 DIVISION VIN BREAKPOINTS CHEV. 88 MODEL YEAR START-UP J (EXCEPT Z24) V-6, 2.8L (W) 25104025 DIVISION VIN BREAKPOINTS CHEV. 88 MODEL YEAR START-UP CADILLAC " " " " L L-4, 2.OL (1) 25103894 DIVISIONS VIN BREAKPOINTS CHEV. JE291207 CHEV. JY280323 CANADA JY805255 L V-6, 2.8L (W) 25103928 DIVISION VIN BREAKPOINTS CHEV. JE260354 CHEV. JY249007 CANADA JY803283 USE APPLICABLE LABOR OPERATION NUMBERS AND LABOR TIME.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.