NEW CAMSHAFT SPROCKET/WRENCH DESIGN - INFORMATION. Chevrolet Corsica 1992

For 1990-2009 cars

# NEW CAMSHAFT SPROCKET/WRENCH DESIGN - INFORMATION

#### SUBJECT: NEW CAMSHAFT SPROCKET AND CAMSHAFT SPROCKET WRENCH DESIGN

VEHICLE APPLICATIONS: 1992 BERETTA ONLY WITH 2.3L ENGINE 1992 Model Year L Cars

ENGINE APPLICATIONS: 2.3L (RPOs LG0)

ENGINE VIN (MODELS): A

#### SERVICE INFORMATION:

Later production 1992 2.3L engines have a powdered metal design camshaft sprocket. To service the new camshaft sprocket requires the camshaft sprocket wrench J 39579. The camshaft sprocket wrench J 39579 is used in the same manner as the previous design, J 36013. Refer to the figure for new sprocket and tool design.

The camshaft sprocket wrench J 39579 will be delivered to dealers in September 1992. Until J 39579 is available, it can be loaned from Kent-Moore by calling 1-800-345-2233.

#### NOTE: Tool availability is limited to dealers with an emergency situation, such as a down vehicle.

When servicing an early 1992 production camshaft sprocket, replace it with the new designed camshaft sprocket, GM P/N 24570973.

Parts are currently available from GMSPO.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.