Low Roller Clutch and Reaction Carrier Disassemble. Chevrolet Corsica 1996

For 1990-2009 cars

1. Remove the following plates from the reaction carrier:

• | The upper low reverse clutch waved plate (688)

• | The low reverse clutch steel and fiber plates (658)

• | The lower low reverse clutch waved plate (688).

• | The selective backing plate (659)

2. Remove the low roller clutch assembly (665) from the reaction internal gear (668).
3. Remove the low roller selective spacer (660) from the reaction carrier assembly (665).
4. Remove the following parts:

• | The low roller race (661)

• | The roller assembly (662)

• | The thrust washer (663)

5. Remove the thrust bearing (667) and the thrust washer (666).