FRONT SEAT BACK TRIM COVER PULLS LOOSE-REPAIR DESCRIBED. Chevrolet Corsica 1988

For 1990-2009 cars

# FRONT SEAT BACK TRIM COVER PULLS LOOSE-REPAIR DESCRIBED

#### Model and Year: 1988 BERETTA

Some cases of seat back trim pulling loose from the seat back on the 1988 Berettas may be reported. To repair this condition use the following procedure:

1. Remove front seat back head restraint and inertia lock knob as described in Section 9L-7 of the Corsica/ Beretta Service Manual.

2. Remove seat back cover.

3. Drill a 3/16" hole through the plastic trim retainer and the metal side frame just above the main side support tube.

4. Install self tapping screw, P/N 20365264 through the plastic trim retainer into seat metal frame.

5. Reinstall seat head restraint, inertia lock knob, and seat back cover.

Labor Operation Number: T1262

Labor Time: .3 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.