W/S REVEAL MOLDING POOR FIT NEW MOLDING P/N AND REPAIR. Chevrolet Corsica 1988

For 1990-2009 cars

# W/S REVEAL MOLDING POOR FIT NEW MOLDING P/N AND REPAIR

MOULDING - WINDSHIELD SIDE -TO- PILLAR REVEAL MOULDING POOR FIT

#### VEHICLES AFFECTED: 1987-88 "L" CAR -----------------

Some comments have been made that the windshield side-to-pillar reveal mouldings have a poor fit at the upper corners on subject vehicles.

Field repairs can be accomplished by installing a revised windshield side-to- pillar reveal moulding per the service procedure below. The part number for the revised mouldings are:

Coupe 10076028-9

Sedan 10076030-1

#### Service Procedure

1. Open front door.

2. Remove sealing strip in area of windshield side reveal moulding.

3. Remove four screws. See Illustration.

4. If necessary, elongate the four holes and slots in the new reveal mouldings so that the moulding end will fit flush to the roof.

5. Install mouldings and reverse the tear down procedure.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.