FRT. DOOR LOCK ROD RATTLES (NEW ANTI-RATTLE CLIPS). Chevrolet Corsica 1988

For 1990-2009 cars

# FRT. DOOR LOCK ROD RATTLES (NEW ANTI-RATTLE CLIPS)

#### Model and Year: 1988-89 L CAR

Customer comments of rattles in the door on 1988-89 L and/or W cars may be the result of loose lock rods in the anti-rattle clips. To correct this condition revised anti-rattle clips should be installed (three anti-rattle clips on coupes, two anti-rattle clips on sedan front per door).

#### Parts required:

Single anti-rattle clip, P/N 16608794 - one required per front door for coupe and sedan.

Double anti-rattle clip, P/N 16609594- two required for coupe, one required for sedan per front door.

Parts are currently available from GMSPO.

#### Service Procedure:

1. Remove trim panel.

2. Remove water deflector to access lock rods.

3. With rods disengaged from anti-rattle clips, grasp clip with pliers and rotate 90 degrees to disengage.

4. Install new anti-rattle clips, reinstall rods.

5. Reinstall water deflector.

6. Reinstall trim panel.

Labor Operation Number: L Car RH T1574 Labor Time: .6 Hours LH T1575 .6 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.