FRT. SHOULDER AND LAP BELT (SERVICE PROCEDURES). Chevrolet Corsica 1988

For 1990-2009 cars

# FRT. SHOULDER AND LAP BELT (SERVICE PROCEDURES)

#### SUBJECT: FRONT SHOULDER BELT AND LAP BELT RETRACTORS AND BELT ASSEMBLY

#### MODEL/YEAR: 1988-90 CORSICA AND BERETTA

Front lap and shoulder belt retractors on passive belt equipped 1988 - 1990 L Coupe and Sedan series will now be serviced individually rather than as complete lap and shoulder belt/retractor assemblies. To service either the lap belt retractor assembly or the shoulder belt retractor assembly, follow the appropriate procedures:

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.