SERVICE MANUAL UPDATE TOWING PROCEDURE. Chevrolet Corsica 1988

For 1990-2009 cars

# SERVICE MANUAL UPDATE TOWING PROCEDURE

TOWING PROCEDURE -SERVICE MANUAL UPDATE

#### Vehicles Affected: 1988 `L' CURRENT TOWING PROCEDURE ----------------- SERVICE MANUAL UPDATE -----------------------

The 1988 Corsica XT will use the current Corsica front tow procedure as stated on page 16 of the 1988 Passenger Car and Light Duty Truck Towing Manual.

The 1988 Corsica must not be towed with sling-type equipment from the rear. Use either wheel-lift equipment and tow up to speeds of 56km/h(35 mph) for no more than 80km(50ml) or use car carrier equipment to transport vehicle.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.